{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Puissance frigorifique","Nom.","","kW","5.00","5.70"]
["Puissance calorifique","Nom.","","kW","6.00","7.00"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","EER","","","3.55","3.48"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","B"]
["Raccords de tuyauterie","Évacuation","OD","mm","VP25 (diamètre ext. : 32 / diamètre int. : 25)","VP25 (diamètre ext. : 32 / diamètre int. : 25)"]
["","Gaz","DE","mm","12.70","12.70"]
["","Liquide","DE","mm","6.35","6.35"]
["Remarques","","","","(1) - En fonctionnement normal : +22°C / +32°C","(1) - En fonctionnement normal : +22°C / +32°C"]
["","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","(4) - Pour les données électriques, se reporter au schéma séparé.","(4) - Pour les données électriques, se reporter au schéma séparé."]