{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Puissance frigorifique","Nom.","","kW","","","","","6.80 (1)","","","","13.4 (1)"]
["Rafraîchissement des locaux","SEER","","","","","","","6.91","6.91","","","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","345","345","","","1,191"]
["","Puissance","Pdesign","kW","","","","","6.80","6.80","","","13.4"]
["","Classe d’efficacité énergétique","","","","","","","A++","A++"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","","","","","7.60","7.60","","","11.8"]
["","SCOP/A","","","","","","","4.54","4.54","","","4.38"]
["","Classe d’efficacité énergétique","","","","","","","A+","A+"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","2,344","2,344","","","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","","","","830"]
["","EER","","","","","","","4.09 (3)","","","","3.18 (3)"]
["","COP","","","","","","","4.80 (3)","","","","4.12 (3)"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","","","","A"]
["","","Chauffage","","","","","","A"]
["Puissance calorifique","Nom.","","kW","","","","","7.50 (2)","","","","15.5 (2)"]
["Remarques","","","","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m"]
["","","","","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m"]
["","","","","","","","","(3) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","","","(3) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["Classe d'efficacité énergétique","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D"]
["Outdoor unit","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","","","","","","","A","A"]
["","Puissance","Pdesign","kW","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","5.10","5.10"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","","","652","824"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","","","","","","","A","A"]
["","Puissance","Pdesign","kW","","","","","","","11.30","12.71"]
["","SCOP/A","","","","","","","","","3.80","3.80"]
["","Pdh Puissance calorifique à -10°","","kW","","","","","","","9.66","11.4"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","","","4164","4683"]