{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":117,"n_cols":9,"rows_kept":117,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["","","","Bas","dBA","","33","35","37"]
["","Rafraîchissement","","Bas","dBA","","33","35","37"]
["","","","Haut","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["Accessoires standard","Manuel d’utilisation","","","","","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation"]
["","Manuel d'installation","","","","","Manuel d'installation","Manuel d'installation","Manuel d'installation"]
["","Flexible d'évacuation","","","","","Flexible d'évacuation","Flexible d'évacuation","Flexible d'évacuation"]
["","Bride pour flexible de vidange","","","","","Bride pour flexible de vidange","Bride pour flexible de vidange","Bride pour flexible de vidange"]
["","Rondelle pour attache de suspension","","","","","Rondelle pour attache de suspension","Rondelle pour attache de suspension","Rondelle pour attache de suspension"]
["","Vis","","","","","Vis","Vis","Vis"]
["","Guide d'installation","","","","","Guide d'installation","Guide d'installation","Guide d'installation"]
["","Isolant pour raccord","","","","","2","2","2"]
["","Tampons d’étanchéité","","","","","4","4","4"]
["","Elément d'étanchéité d’évacuation","","","","","Elément d'étanchéité d’évacuation","Elément d'étanchéité d’évacuation","Elément d'étanchéité d’évacuation"]
["","Attaches","","","","","Attaches","Attaches","Attaches"]
["Systèmes de commande","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Raccords de tuyauterie","Liquide","","DE","mm","","9.52","9.52","9.52"]
["","Gaz","","DE","mm","","15.9","15.9","15.9"]
["","Évacuation","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Panneau décoratif 4","Dimensions","","Profondeur","mm","","50","50","50"]
["","","","Largeur","mm","","950","950","950"]
["","","","Hauteur","mm","","950","950","950"]
["","Modèle","","","","","BYCQ140D7W1 - blanc à déflecteurs gris","BYCQ140D7W1 - blanc à déflecteurs gris","BYCQ140D7W1 - blanc à déflecteurs gris"]
["","Couleur","","","","","Blanc pur (RAL 9010)","Blanc pur (RAL 9010)","Blanc pur (RAL 9010)"]
["","Poids","","","kg","","5.4","5.4","5.4"]
["Sound power level","Rafraîchissement","","","dBA","","61","61","61"]
["","Chauffage","","","dBA","","61","61","61"]
["Dimensions","Unité","","Largeur","mm","","840","840","840"]
["","","","Profondeur","mm","","840","840","840"]
["","","","Hauteur","mm","","288","288","288"]
["Caisson","Matériau","","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Poids","Unité","","","kg","","26","26","26"]
["Panneau décoratif","Poids","","","kg","","10.3","10.3","10.3"]
["","Modèle","","","","","BYCQ140D7GFW1 - panneau autonettoyant à filtre à mailles fines","BYCQ140D7GFW1 - panneau autonettoyant à filtre à mailles fines","BYCQ140D7GFW1 - panneau autonettoyant à filtre à mailles fines"]
["","Dimensions","","Hauteur","mm","","130","130","130"]
["","","","Profondeur","mm","","950","950","950"]
["","","","Largeur","mm","","950","950","950"]
["","Couleur","","","","","Blanc pur (RAL 9010)","Blanc pur (RAL 9010)","Blanc pur (RAL 9010)"]
["Power supply","Phase","","","","","1~","1~","1~"]
["","Fréquence","","","Hz","","50","50","50"]
["","Nom","","","","","VE","VE","VE"]
["","Tension","","","V","","220-240","220-240","220-240"]
["Remarques","","","","","","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore."]
["","","","","","","(2) - Le modèle BYCQ140D7W1W est doté de matériaux d'isolation blancs. Il est à noter que l'accumulation de saletés sur un matériau d'isolation blanc est bien visible. Il est par conséquent déconseillé d'installer le panneau décoratif BYCQ140D7W1W dans des environnements exposés à de fortes concentrations de saletés.","(2) - Le modèle BYCQ140D7W1W est doté de matériaux d'isolation blancs. Il est à noter que l'accumulation de saletés sur un matériau d'isolation blanc est bien visible. Il est par conséquent déconseillé d'installer le panneau décoratif BYCQ140D7W1W dans des environnements exposés à de fortes concentrations de saletés.","(2) - Le modèle BYCQ140D7W1W est doté de matériaux d'isolation blancs. Il est à noter que l'accumulation de saletés sur un matériau d'isolation blanc est bien visible. Il est par conséquent déconseillé d'installer le panneau décoratif BYCQ140D7W1W dans des environnements exposés à de fortes concentrations de saletés."]
["","","","","","","(3) - BYCQ140D7W1 : panneau standard blanc pur à déflecteurs gris ; BYCQ140D7W1W : panneau standard blanc pur à déflecteurs blancs ; BYCQ140D7GW1 : panneau autonettoyant blanc pur.","(3) - BYCQ140D7W1 : panneau standard blanc pur à déflecteurs gris ; BYCQ140D7W1W : panneau standard blanc pur à déflecteurs blancs ; BYCQ140D7GW1 : panneau autonettoyant blanc pur.","(3) - BYCQ140D7W1 : panneau standard blanc pur à déflecteurs gris ; BYCQ140D7W1W : panneau standard blanc pur à déflecteurs blancs ; BYCQ140D7GW1 : panneau autonettoyant blanc pur."]
["Caisson","Matériau","","","","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","288"]
["","","","Largeur","mm","840"]
["","","","Profondeur","mm","840"]
["Poids","Unité","","","kg","25"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Bas","m³/min","12.2"]
["","","Chauffage","Haut","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Bas","m³/min","12.2"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","53"]
["","Chauffage","","","dBA","53"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Bas","dBA","29"]
["","Chauffage","","Haut","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Bas","dBA","29"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52"]
["","Gaz","","DE","mm","15.9"]
["","Évacuation","","","","VP25 (I.D. 25/O.D. 32)"]
["Panneau décoratif","Modèle","","","","BYCQ140D7GFW1 - panneau autonettoyant à filtre à mailles fines"]
["","Couleur","","","","Blanc pur (RAL 9010)"]
["","Dimensions","","Hauteur","mm","130"]
["","","","Largeur","mm","950"]
["","","","Profondeur","mm","950"]
["","Poids","","","kg","10.3"]
["Panneau décoratif&nbsp;2","Panneau décoratif&nbsp;2-=-Modèle","","","","BYCQ140D7GW1 - Panneau auto-nettoyant"]
["","Panneau décoratif&nbsp;2-=-Couleur","","","","Blanc pur (RAL 9010)"]
["","Panneau décoratif&nbsp;2-=-Dimensions","","Panneau décoratif&nbsp;2-=-Dimensions-=-Hauteur-=-mm","mm","130"]
["","","","Panneau décoratif&nbsp;2-=-Dimensions-=-Largeur-=-mm","mm","950"]
["","","","Panneau décoratif&nbsp;2-=-Dimensions-=-Profondeur-=-mm","mm","950"]
["","Panneau décoratif&nbsp;2-=-Poids-=-kg","","","kg","10.3"]
["Panneau décoratif&nbsp;3","Panneau décoratif&nbsp;3-=-Modèle","","","","BYCQ140D7W1W - Totalement blanc"]
["","Panneau décoratif&nbsp;3-=-Couleur","","","","Blanc pur (RAL 9010)"]
["","Panneau décoratif&nbsp;3-=-Dimensions","","Panneau décoratif&nbsp;3-=-Dimensions-=-Hauteur-=-mm","mm","50"]
["","","","Panneau décoratif&nbsp;3-=-Dimensions-=-Largeur-=-mm","mm","950"]
["","","","Panneau décoratif&nbsp;3-=-Dimensions-=-Profondeur-=-mm","mm","950"]
["","Panneau décoratif&nbsp;3-=-Poids-=-kg","","","kg","5.4"]
["Panneau décoratif&nbsp;4","Panneau décoratif&nbsp;4-=-Modèle","","","","BYCQ140D7W1 - Blanc avec déflecteurs gris"]
["","Panneau décoratif&nbsp;4-=-Couleur","","","","Blanc pur (RAL 9010)"]
["","Panneau décoratif&nbsp;4-=-Dimensions","","Panneau décoratif&nbsp;4-=-Dimensions-=-Hauteur-=-mm","mm","950"]
["","","","Panneau décoratif&nbsp;4-=-Dimensions-=-Largeur-=-mm","mm","950"]
["","","","Panneau décoratif&nbsp;4-=-Dimensions-=-Profondeur-=-mm","mm","50"]
["","Panneau décoratif&nbsp;4-=-Poids-=-kg","","","kg","5.4"]
["Systèmes de commande","Infrared remote control","","","","BRC7FA532F"]
["Systèmes de commande","Télécommande câblée","","","","BRC1D52, BRC1E52A/B"]
["Accessoires standard","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Alimentation électrique","Nom","","","","VE"]
["","Phase","","","","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50"]
["","Alimentation électrique-=-Tension","","Alimentation électrique-=-Tension-=-V","","220-240"]