{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZQ-C"]
[]
[]
[]
[]
["","","","","FDA200AXVEB / RZQ200C7Y1B","FDA250AXVEB / RZQ250C7Y1B"]
["Puissance frigorifique","Nom.","","kW","19.0 (1)","22.0 (1)"]
["Rafraîchissement des locaux","SEER","","","4.60","4.60"]
["","Consommation d’énergie annuelle","","kWh/a","2,478","2,869"]
["","Puissance","Pdesign","kW","19.0","22.0"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","16.7","17.5"]
["","SCOP/A","","","3.40","3.40"]
["","Consommation d’énergie annuelle","","kWh/a","6,875","7,205"]
["Puissance calorifique","Nom.","","kW","22.4 (2)","24.0 (2)"]
["Remarques","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m"]
["","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m"]
["","","","","(3) - Cette valeur n’inclut pas la baisse de puissance due au dégivrage.","(3) - Cette valeur n’inclut pas la baisse de puissance due au dégivrage."]