{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Puissance frigorifique","Min.","","kW","","1.70"]
["","Nom.","","kW","","6.00"]
["","Max.","","kW","","6.50"]
["Puissance calorifique","Min.","","kW","","1.70"]
["","Nom.","","kW","","7.00"]
["","Max.","","kW","","7.10"]
["Efficacité nominale","EER","","","","2.93"]
["","COP","","","","3.21"]
["","Consommation énergétique annuelle","","kWh","","1,024"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","C"]
["","","Chauffage","","","C"]
["Rafraîchissement de l'air ambiant","Classe d’efficacité énergétique","","","","A"]
["","Puissance","Pdesign","kW","","6.00"]
["","SEER","","","","5.56"]
["","Consommation d’énergie annuelle","","kWh/a","","378"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","","A"]
["","Puissance","Pdesign","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","Consommation d’énergie annuelle","","kWh/a","","1,693"]
["Remarques","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(2) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","","(4) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Puissance frigorifique","Min.","","kW","1.70"]
["","Nom.","","kW","5.00"]
["","Max.","","kW","5.30"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.70"]
["","Nom.","","kW","5.80"]
["","Max.","","kW","6.00"]
["Efficacité nominale","EER","","","3.06"]
["","COP","","","3.10"]
["","Consommation énergétique annuelle","","kWh","816"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","B"]
["","","Chauffage","","D"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+"]
["","Puissance","Pdesign","kW","5.00"]
["","SEER","","","5.77"]
["","Consommation d’énergie annuelle","","kWh/a","303"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A"]
["","Puissance","Pdesign","kW","4.00"]
["","SCOP/A","","","3.93"]
["","Pdh Puissance calorifique à -10°","","kW","3.55"]
["","Consommation d’énergie annuelle","","kWh/a","1424"]
["Classe d'efficacité énergétique","","","","A+++ ~ D"]