{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Puissance frigorifique","Min.","","kW","1.2"]
["","Max.","","kW","3.8"]
["","Nom.","","kW","3.5"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35"]
["","Gaz","DE","mm","9.5"]
["","Évacuation","DE","mm","18.0"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","B"]
["","","Chauffage","","B"]
["Puissance calorifique","Nom.","","kW","4.0"]
["","Min.","","kW","1.4"]
["","Max.","","kW","5.0"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - 220V"]
["","","","","(3) - 230 V"]
["","","","","(4) - 240V"]
["","","","","(5) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m"]
["","","","","(6) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["","","","","(7) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]