{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-KN"]
[]
[]
[]
[]
["","","","","FTX25KNV1B","FTX35KNV1B"]
["Niveau de pression sonore","Chauffage","Haut","dBA","40","43"]
["","","Moyen","dBA","34","35"]
["","","Faible niveau sonore de fonctionnement","dBA","25","26"]
["","","Bas","dBA","28","29"]
["","Rafraîchissement","Moyen","dBA","33","34"]
["","","Faible niveau sonore de fonctionnement","dBA","20","20"]
["","","Bas","dBA","26","27"]
["","","Haut","dBA","40","43"]
["","","Nom.","dBA","34","35"]
["","Rafraîchissement","Nom.","dBA","33","34"]
["Accessoires standard","Manuel d'installation","","","1","1"]
["","Manuel d’utilisation","","","1","1"]
["","Télécommande infrarouge","","","1","1"]
["","Piles sèches AA","","","2","2"]
["","Support de télécommande","","","1","1"]
["","Plaque de montage","","","1","1"]
["","Filtre purificateur d'air photocatalytique à apatite de titane","","","2","2"]
["","Vis de fixation d'unité intérieure","","","2","2"]
["Systèmes de contrôle","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.5"]
["","Évacuation","","","18","18"]
["Sound power level","Rafraîchissement","","dBA","55","55"]
["","Chauffage","","dBA","55","56"]
["Dimensions","Unité","Largeur","mm","770","770"]
["","","Profondeur","mm","225","225"]
["","","Hauteur","mm","285","285"]
["Caisson","Couleur","","","Blanc","Blanc"]
["Poids","Unité","","kg","8.5","9"]
["Power supply","Phase","","","1~","1~"]
["","Fréquence","","Hz","50","50"]
["","Nom","","","V1","V1"]
["","Tension","","V","220-240","220-240"]