{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":10,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXB-B"]
[]
[]
[]
[]
["","","","","FTXB25B1V1","FTXB25BV1","FTXB35BV1","FTXB35B1V1","FTXB50BV1B","FTXB60BV1B"]
["Niveau de pression sonore","Chauffage","Haut","dBA","38","38","40","40","40","43"]
["","","Moyen","dBA","33","","","34"]
["","","Faible niveau sonore de fonctionnement","dBA","25","25","23","23","32","33"]
["","","Bas","dBA","28","28","26","26","35","37"]
["","Rafraîchissement","Moyen","dBA","33","","","34"]
["","","Faible niveau sonore de fonctionnement","dBA","22","22","25","25","32","33"]
["","","Très élevé","dBA","","","","","44","46"]
["","","Bas","dBA","25","25","26","26","35","37"]
["","","Haut","dBA","38","38","39","39","40","43"]
["","","Nom.","dBA","33","33","34","34","38","41"]
["","Rafraîchissement","Nom.","dBA","33","33","34","34","38","41"]
["Accessoires standard","Manuel d'installation","","","1","1","1","1"]
["","Manuel d’utilisation","","","1","1","1","1"]
["","Télécommande infrarouge","","","1","1","1","1"]
["","Piles sèches AA","","","2","","","2"]
["","Support de télécommande","","","1","1","1","1"]
["","Plaque de montage","","","1","1","1","1"]
["","Vis de fixation d'unité intérieure","","","2","2","2","2"]
["Systèmes de commande","Infrared remote control","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","APGS02","APGS02"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.5","9.5","9.5"]
["","Évacuation","","","18","18","18","18"]
["Puissance absorbée","Rafraîchissement","Nom.","kW","0.030","0.040","0.040","0.030"]
["","Chauffage","Nom.","kW","0.040","0.040","0.040","0.040"]
["Niveau de puissance sonore","Rafraîchissement","","dBA","52","52","53","53","55","61"]
["","Chauffage","","dBA","52","52","54","54"]
["Dimensions","Unité","Largeur","mm","770","770","770","770","1,065","1,065"]
["","","Profondeur","mm","216","216","216","216","224","224"]
["","","Hauteur","mm","283","283","283","283","310","310"]
["Caisson","Couleur","","","","","","","Blanc","Blanc"]
["Poids","Unité","","kg","7","8","8","7","14","14"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","Hz","50","50","50","50","50","50"]
["","Nom","","","V1","V1","V1","V1","V1","V1"]
["","Tension","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Remarques","","","","(1) - Contient des gaz à effet de serre fluorés.","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - Contient des gaz à effet de serre fluorés."]
["Accessoires standard","Piles","","","","2","2"]
["","Filtre purificateur d'air photocatalytique à apatite de titane","","","","2","2"]
["Remarques","","","","","","","","(1) - Toutes les unités sont testées et conformes à la norme ISO5151 (unité non gainée) ou ISO13253 (unité gainée)","(1) - Toutes les unités sont testées et conformes à la norme ISO5151 (unité non gainée) ou ISO13253 (unité gainée)"]
["","","","","","","","","(2) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis.","(2) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis."]