{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D / RXF-D9"]
[]
[]
[]
[]
["","","","","FTXF60D2V1B / RXF60D5V1B9","FTXF71D2V1B / RXF71D5V1B9"]
["Puissance frigorifique","Min.","","kW","1.7","2.3"]
["","Nom.","","kW","6","7.1"]
["","Max.","","kW","7","7.3"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.7","2.3"]
["","Nom.","","kW","6.4","8.2"]
["","Max.","","kW","8","9"]
["Efficacité nominale","EER","","","3.25","2.56"]
["","COP","","","3.93","3.15"]
["","Consommation énergétique annuelle","","kWh","923","1387"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","E"]
["","","Chauffage","","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++","A"]
["","Puissance","Pdesign","kW","6","7.1"]
["","SEER","","","6.15","5.15"]
["","Consommation d’énergie annuelle","","kWh/a","342","483"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+","A"]
["","Puissance","Pdesign","kW","4.8","6.2"]
["","SCOP/A","","","4.06","3.81"]
["","Pdh Puissance calorifique à -10°","","kW","4.24","5.02"]
["","Consommation d’énergie annuelle","","kWh/a","1654","2275"]
["Remarques","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]