{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":7,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JB"]
[]
[]
[]
[]
["","","","","FTXG25JV1BB","FTXG35JV1BB","FTXG50JV1BB"]
["Niveau de pression sonore","Chauffage","Haut","dBA","39","42","44"]
["","","Faible niveau sonore de fonctionnement","dBA","25","26","32"]
["","","Bas","dBA","28","29","35"]
["","Rafraîchissement","Faible niveau sonore de fonctionnement","dBA","22","23","32"]
["","","Bas","dBA","25","26","35"]
["","","Haut","dBA","38","42","44"]
["","","Nom.","dBA","34","36","40"]
["","Rafraîchissement","Nom.","dBA","32","34","40"]
["Accessoires standard","Filtre purificateur d'air photocatalytique à apatite de titane","","","2","2","2"]
["","Manuel d’utilisation","","","1","1","1"]
["","Manuel d'installation","","","1","1","1"]
["","Télécommande infrarouge","","","1","1","1"]
["","Piles","","","2","2","2"]
["","Support de télécommande","","","1","1","1"]
["","Vis de fixation d'unité intérieure","","","2","2","2"]
["","Plaque de montage","","","1","1","1"]
["","Schéma papier","","","2","2","2"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35"]
["","Gaz","DE","mm","9.52","9.52","12.7"]
["","Drain","","","16 ou 18","16 ou 18","18"]
["Puissance absorbée","Rafraîchissement","Nom.","kW","0.018 (3), 0.018 (4), 0.018 (5)","0.026 (3), 0.026 (4), 0.026 (5)","0.032 (3), 0.032 (4), 0.032 (5)"]
["","Chauffage","Nom.","kW","0.024 (3), 0.024 (4), 0.024 (5)","0.032 (3), 0.032 (4), 0.032 (5)","0.038 (3), 0.038 (4), 0.038 (5)"]
["Niveau de puissance sonore","Rafraîchissement","","dBA","56","60","60"]
["","Chauffage","","dBA","57","60","60"]
["Dimensions","Unité","Largeur","mm","915","915","915"]
["","","Profondeur","mm","155","155","155"]
["","","Hauteur","mm","295","295","295"]
["Caisson","Colour","","","Noir mat","Noir mat","Noir mat"]
["Poids","Unité","","kg","11","11","11"]
["Power supply","Phase","","","1~","1~","1~"]
["","Fréquence","","Hz","50","50","50"]
["","Nom","","","V1","V1","V1"]
["","Tension","","V","220-240","220-240","220-240"]
["Remarques","","","","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)"]
["","","","","(2) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder.","(2) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder.","(2) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder."]
["","","","","(3) - 220V","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230 V","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240V","(5) - 240V","(5) - 240V"]