{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Niveau de pression sonore","Chauffage","Haut","dBA","47","47"]
["","","Faible niveau sonore de fonctionnement","dBA","19","19"]
["","","Bas","dBA","23","23"]
["","Rafraîchissement","Faible niveau sonore de fonctionnement","dBA","21","21"]
["","","Bas","dBA","33","33"]
["","","Haut","dBA","45","45"]
["","","Nom.","dBA","37","36"]
["","Rafraîchissement","Nom.","dBA","39","39"]
["Accessoires standard","Manuel d'installation","","","1","1"]
["","Manuel d’utilisation","","","1","1"]
["","Télécommande infrarouge","","","1","1"]
["","Piles","","","2","2"]
["","Support de télécommande","","","1","1"]
["","Plaque de montage","","","1","1"]
["","Filtre purificateur d'air photocatalytique à apatite de titane","","","2","2"]
["","Vis de fixation d'unité intérieure","","","2","2"]
["Systèmes de commande","Infrared remote control","","","ARC466A9","ARC466A9"]
["Raccordements de tuyauterie","Liquide","DE","mm","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.5"]
["","Évacuation","","","18","18"]
["Power input","Rafraîchissement","Nom.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Chauffage","Nom.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Rafraîchissement","","dBA","59","59"]
["","Chauffage","","dBA","62","62"]
["Dimensions","Unité","Largeur","mm","900","900"]
["","","Profondeur","mm","215","215"]
["","","Hauteur","mm","298","298"]
["Caisson","Couleur","","","Blanc","Blanc"]
["Poids","Unité","","kg","12","12"]
["Power supply","Phase","","","1~","1~"]
["","Fréquence","","Hz","50","50"]
["","Nom","","","V1","V1"]
["","Tension","","V","220-240","220-240"]
["Remarques","","","","(1) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder.","(1) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240V","(4) - 240V"]