{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 2MXM-M9"]
[]
[]
[]
[]
["","","","","FTXM25M2V1B / FTXM42M2V1B / 2MXM50M2V1B9"]
["Puissance frigorifique","Nom.","","kW","5.0"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","612"]
["","EER","","","4.09"]
["","COP","","","4.03"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A"]
["","","Chauffage","","A"]
["Puissance calorifique","Min.","","kW","5.60"]
["Remarques","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes: temp.intérieure:27°CBS,19°CBH; temp.extérieure:35°CBS; longueur équivalente de tuyauterie de réfrigérant:5m, dénivellation:0m. Données pour des séries d'efficacité standard. Utilisation des tolérances Eurovent2015."]
["","","","","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]