{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M"]
[]
[]
[]
[]
["","","","","","FTXM20M2V1B","FTXM25M2V1B","FTXM35M2V1B","FTXM42M2V1B","FTXM50M2V1B","FTXM60M2V1B","FTXM71M2V1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.03","0.03","0.035","0.035","0.03","0.032","0.054"]
["","Chauffage","","Nom.","kW","0.025","0.025","0.025","0.035","0.032","0.035","0.06"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","294","294","294","294","300","300","300"]
["","","","Largeur","mm","811","811","811","811","1040","1040","1040"]
["","","","Profondeur","mm","272","272","272","272","295","295","295"]
["Poids","Unité","","","kg","10","10","10","10","14.5","14.5","14.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","11.1","11.1","12.6","12.6","16.5","17.1","17.6"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","7.9","8.1","8.3","9.5","14.2","14.6","15"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6","6.2","6.4","7.1","11.6","12","12.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.4","4.4","4.6","4.6","10.3","10.7","11.1"]
["","","Chauffage","Haut","m³/min","10.4","10.4","10.4","13","17.1","17.7","18.4"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.7","8.7","9","10.4","14.6","15.6","16.2"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.5","6.8","7.1","7.1","12.2","12.6","13"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.3","5.3","5.3","5.3","10.7","11.2","11.9"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","57","57","60","60","59","60","60"]
["","Chauffage","","","dBA","54","54","54","60","58","59","61"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","41","41","45","45","44","46","47"]
["","Refroidissement","","Moyen","dBA","33","33","33","39","40","42","43"]
["","","","Bas","dBA","25","25","29","30","36","37","38"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19","19","21","32","34","35"]
["","Chauffage","","Haut","dBA","39","39","39","45","43","45","46"]
["","","","Moyen","dBA","34","34","35","39","39","41","42"]
["","","","Bas","dBA","26","27","28","29","34","36","37"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","20","20","21","31","33","34"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.5","9.5","9.5","12.7","12.7","12.7","15.9"]
["","Évacuation","","","","18","18","18","18","18","18","18"]
["Systèmes de commande","Infrared remote control","","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Systèmes de commande","Télécommande câblée","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073","BRC944B2, BRC073","BRC944B2, BRC073"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1"]
["Alimentation électrique","Nom","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Systèmes de commande","Télécommande infrarouge","","","","","","","","","ARC466A33","ARC466A33"]