{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N9 / RXP-N9"]
[]
[]
[]
[]
["","","","","FTXP20N5V1B9 / RXP20N5V1B9 (Archived)","FTXP25N5V1B9 / RXP25N5V1B9 (Archived)","FTXP35N5V1B9 / RXP35N5V1B9 (Archived)"]
["Outdoor unit","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9"]
["Puissance frigorifique","Min.","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2","2.5","3.5"]
["","Max.","","kW","2.6","3","4"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2.5","3","4"]
["","Max.","","kW","3.5","4","4.8"]
["Efficacité nominale","EER","","","3.75","3.75","3.48"]
["","COP","","","4.77","4.36","4.02"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A","A"]
["","","Chauffage","","A","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++","A++","A++"]
["","Puissance","Pdesign","kW","2","2.5","3.5"]
["","SEER","","","7.2","7.2","7.2"]
["","Consommation d’énergie annuelle","","kWh/a","97","121","170"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A++","A++","A++"]
["","Puissance","Pdesign","kW","2.2","2.4","2.8"]
["","SCOP/A","","","4.65","4.61","4.64"]
["","Pdh Puissance calorifique à -10°","","kW","1.99","2.09","2.35"]
["","Consommation d’énergie annuelle","","kWh/a","663","728","845"]
["Remarques","","","","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(2) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(2) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]