{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N9"]
[]
[]
[]
[]
["","","","","","FTXP35N5V1B9","FTXP50N5V1B9","FTXP20N5V1B9 (Archived)"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.032","0.04","0.021"]
["","Chauffage","","Nom.","kW","0.032","0.04","0.023"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","286","286","286"]
["","","","Largeur","mm","770","770","770"]
["","","","Profondeur","mm","225","225","225"]
["Poids","Unité","","","kg","9","9","9"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","11.5","11.8","9.6"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8.3","9.3","7.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6.3","7.6","5.6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.5","6","4.4"]
["","","Chauffage","Haut","m³/min","11.5","11.9","10.6"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","9","9.5","8.6"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","7","8.2","6.6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.1","7.4","5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","58","59","55"]
["","Chauffage","","","dBA","58","61","55"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","43","46","39"]
["","Refroidissement","","Moyen","dBA","34","39","33"]
["","","","Bas","dBA","27","34","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","27","19"]
["","Chauffage","","Haut","dBA","40","44","39"]
["","","","Moyen","dBA","35","38","34"]
["","","","Bas","dBA","29","33","28"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","30","21"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.52","12.7","9.52"]
["","Évacuation","","","","18","18","18"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Télécommande câblée","","","","BRC073A1","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1"]
["","Silver particle filter","","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240"]
["Remarques","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Rafraîchissement: temp. intérieure 27°CBS, 19°CBH; temp. extérieure 35°CBS; longueur équivalente de tuyauterie : 5m; dénivelé: 0m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Chauffage: temp. intérieure 20°CBS; temp. extérieure 7°CBS, 6°CBH ; tuyauterie équivalente de réfrigérant : 5m (horizontale)"]
["","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - Pour les données électriques, se reporter au schéma séparé."]