{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB / RXTA-B"]
[]
[]
[]
[]
["","","","","FTXTA30B2V1BB / RXTA30B2V1B"]
["Puissance frigorifique","Min.","","kW","0.70"]
["","Nom.","","kW","3.00"]
["","Max.","","kW","4.50"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","0.80"]
["","Nom.","","kW","3.20"]
["","Max.","","kW","6.90"]
["Efficacité nominale","EER","","","4.20"]
["","COP","","","4.87"]
["","Consommation énergétique annuelle","","kWh","357"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A"]
["","","Chauffage","","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++"]
["","Puissance","Pdesign","kW","3.00"]
["","SEER","","","7.63"]
["","Consommation d’énergie annuelle","","kWh/a","138"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+++"]
["","Puissance","Pdesign","kW","2.60"]
["","SCOP/A","","","5.10"]
["","Pdh Puissance calorifique à -10°","","kW","2.60"]
["","Consommation d’énergie annuelle","","kWh/a","714"]
["Classe d'efficacité énergétique","","","","A+++ ~ D"]