{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-DY"]
[]
[]
[]
[]
["","","","","","FTXTA30D2V1BY"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.023"]
["","Chauffage","","Nom.","kW","0.022"]
["Caisson","Couleur","","","","Casing: Black, Panel: Dark wood "]
["Dimensions","Unité","","Hauteur","mm","295"]
["","","","Largeur","mm","798"]
["","","","Profondeur","mm","189"]
["Poids","Unité","","","kg","12"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","13.1"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","9.0"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6.0"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.9"]
["","","Chauffage","Haut","m³/min","12.3"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.2"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","5.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.0"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60"]
["","Chauffage","","","dBA","60"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","43"]
["","Refroidissement","","Moyen","dBA","32"]
["","","","Bas","dBA","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","20"]
["","Chauffage","","Haut","dBA","41"]
["","","","Moyen","dBA","31"]
["","","","Bas","dBA","24"]
["","","","Faible niveau sonore de fonctionnement","dBA","19"]
["Réfrigérant","Réfrigérant-=-PRP","","","","675.0"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.50"]
["","Évacuation","","","","18"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A95"]
["","Télécommande câblée","","","","BRC073A1"]
["Accessoires standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Classe d'efficacité énergétique","","","","","A+++ ~ D"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240"]
["Remarques","","","","","(1) - Rafraîchissement: temp. intérieure 27°CBS, 19°CBH; temp. extérieure 35°CBS, 24°CBH; longueur équivalente de tuyauterie : 5m"]
["","","","","","(2) - Chauffage: temp. intérieure 20°CBS; temp. extérieure 7°CBS, 6°CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["","","","","","(3) - Pour les données électriques, se reporter au schéma séparé."]