{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.035","0.053"]
["","Chauffage","","Nom.","kW","0.039","0.06"]
["Caisson","Couleur","","","","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","295","299"]
["","","","Largeur","mm","778","998"]
["","","","Profondeur","mm","272","292"]
["Poids","Unité","","","kg","10","15"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","11.5","15.1"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","7.5","9.2"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","5.2","5.6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.2","4.8"]
["","","Chauffage","Haut","m³/min","11.6","17"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","7.3","10"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","4.7","6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4","5.1"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60","60"]
["","Chauffage","","","dBA","60","60"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","45","46"]
["","Refroidissement","","Moyen","dBA","33","32"]
["","","","Bas","dBA","25","24"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","20"]
["","Chauffage","","Haut","dBA","45","46"]
["","","","Moyen","dBA","31","31"]
["","","","Bas","dBA","22","22"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19"]
["Réfrigérant","Réfrigérant-=-PRP","","","","675","675"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35"]
["","Gaz","","DE","mm","9.5","9.5"]
["","Évacuation","","","","18","18"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A83","ARC466A83"]
["","Télécommande câblée","","","","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]