{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A / RXTP-A"]
[]
[]
[]
[]
["","","","","FTXTP25A5V1B / RXTP25A2V1B","FTXTP35A5V1B / RXTP35A2V1B"]
["Puissance frigorifique","Min.","","kW","1","1"]
["","Nom.","","kW","2.5","3.5"]
["","Max.","","kW","4.1","4.5"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1","1"]
["","Nom.","","kW","3.2","4"]
["","Max.","","kW","6.2","6.7"]
["Efficacité nominale","EER","","","4.88","4.71"]
["","COP","","","4.99","4.55"]
["","Consommation énergétique annuelle","","kWh","256","372"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","2.5","3.5"]
["","SEER","","","8.55","8.55"]
["","Consommation d’énergie annuelle","","kWh/a","102","143"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A++","A++"]
["","Puissance","Pdesign","kW","2.5","3"]
["","SCOP/A","","","4.95","4.85"]
["","Pdh Puissance calorifique à -10°","","kW","2.5","3"]
["","Consommation d’énergie annuelle","","kWh/a","707","866"]
["Remarques","","","","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(2) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]