{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","43"]
["","","","Moyen","dBA","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","21"]
["","","","Bas","dBA","26"]
["","Rafraîchissement","","Moyen","dBA","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","21"]
["","","","Bas","dBA","26"]
["","","","Haut","dBA","43"]
["Accessoires standard","Manuel d'installation","","","","1"]
["","Manuel d’utilisation","","","","1"]
["","Télécommande infrarouge","","","","1"]
["","Piles sèches AAA","","","","2"]
["","Support de télécommande","","","","1"]
["","Plaque de montage","","","","1"]
["","Filtre désodorisant à apatite de titane","","","","2"]
["","Vis de fixation d'unité intérieure","","","","2"]
["Systèmes de commande","Télécommande câblée","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Piping connections","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.50"]
["","Drain","","","","16 (diamètre interne du flexible de raccordement)"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.030"]
["","Chauffage","","Nom.","kW","0.035"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","58"]
["","Chauffage","","","dBA","58"]
["Dimensions","Unité","","Largeur","mm","770"]
["","","","Profondeur","mm","225"]
["","","","Hauteur","mm","285"]
["Caisson","Colour","","","","Blanc"]
["Poids","Unité","","","kg","9.0"]
["Power supply","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Nom","","","","V1"]
["","Tension","","","V","220-240"]
["Remarques","","","","","(1) - Pour les données électriques, se reporter au schéma séparé."]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.03"]
["","Chauffage","","Nom.","kW","","0.035"]
["Caisson","Couleur","","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","285"]
["","","","Largeur","mm","","770"]
["","","","Profondeur","mm","","225"]
["Poids","Unité","","","kg","","9"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","11.4"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","8.2"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","5.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","4.3"]
["","","Chauffage","Haut","m³/min","","10.8"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","7.8"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","5.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","4.9"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","58"]
["","Chauffage","","","dBA","","58"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","43"]
["","Refroidissement","","Moyen","dBA","","35"]
["","","","Bas","dBA","","26"]
["","","","Faible niveau sonore de fonctionnement","dBA","","21"]
["","Chauffage","","Haut","dBA","","43"]
["","","","Moyen","dBA","","35"]
["","","","Bas","dBA","","26"]
["","","","Faible niveau sonore de fonctionnement","dBA","","21"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35"]
["","Gaz","","DE","mm","","9.5"]
["","Évacuation","","","","","16 (diamètre interne du flexible de raccordement)"]
["Systèmes de commande","Infrared remote control","","","","","ARC480A11"]
["Systèmes de commande","Télécommande câblée","","","","","BRC944B2, BRC073A1"]
["Accessoires standard","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Alimentation électrique","Nom","","","","","V1"]
["","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240"]