{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Niveau de pression sonore","Chauffage","Haut","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["","","Bas","dBA","35","39","40"]
["","Rafraîchissement","Bas","dBA","35","39","40"]
["","","Haut","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["Accessoires standard","Manuel d'installation","","","Manuel d'installation","Manuel d'installation","Manuel d'installation"]
["","Manuel d’utilisation","","","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation"]
["","Déclaration de conformité","","","Déclaration de conformité","Déclaration de conformité","Déclaration de conformité"]
["","Flexible d'évacuation","","","Flexible d'évacuation","Flexible d'évacuation","Flexible d'évacuation"]
["","Attache métallique","","","Attache métallique","Attache métallique","Attache métallique"]
["","Rondelle pour attache de suspension","","","Rondelle pour attache de suspension","Rondelle pour attache de suspension","Rondelle pour attache de suspension"]
["","Attaches","","","Attaches","Attaches","Attaches"]
["","Rondelle de serrage","","","Rondelle de serrage","Rondelle de serrage","Rondelle de serrage"]
["","Matériau d'étanchéité et d'isolation pour raccord","","","Matériau d'étanchéité et d'isolation pour raccord","Matériau d'étanchéité et d'isolation pour raccord","Matériau d'étanchéité et d'isolation pour raccord"]
["","Coude","","","Coude","Coude","Coude"]
["","Schéma d’installation","","","Schéma d’installation","Schéma d’installation","Schéma d’installation"]
["","Matériau de blocage","","","Matériau de blocage","Matériau de blocage","Matériau de blocage"]
["","Tuyauterie en L","","","Tuyauterie en L","Tuyauterie en L","Tuyauterie en L"]
["","Vis","","","Vis","Vis","Vis"]
["","Tissu non tissé","","","Tissu non tissé","Tissu non tissé","Tissu non tissé"]
["Systèmes de commande","Télécommande câblée","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Raccordements de tuyauterie","Liquide","DE","mm","9.52","9.52","9.52"]
["","Gaz","DE","mm","15.9","15.9","15.9"]
["","Évacuation","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Rafraîchissement","","dBA","59","64","65"]
["","Chauffage","","dBA","59","64","65"]
["Dimensions","Unité","Largeur","mm","950","950","950"]
["","","Profondeur","mm","950","950","950"]
["","","Hauteur","mm","198","198","198"]
["Caisson","Matériau","","","Résine","Résine","Résine"]
["","Couleur","","","Blanc frais","Blanc frais","Blanc frais"]
["Poids","Unité","","kg","25","26","26"]
["Hauteur manométrique","mm","","","600","600","600"]
["Power supply","Phase","","","1~","1~","1~"]
["","Fréquence","","Hz","50/60","50/60","50/60"]
["","Nom","","","VE","VE","VE"]
["","Tension","","V","220-240/220","220-240/220","220-240/220"]