{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Niveau de pression sonore","Chauffage","Haut","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["","","Bas","dBA","38","44","46","48"]
["","Rafraîchissement","Bas","dBA","38","44","46","48"]
["","","Haut","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["Accessoires standard","Manuel d’utilisation","","","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation"]
["","Manuel d'installation","","","Manuel d'installation","Manuel d'installation","Manuel d'installation","Manuel d'installation"]
["","Support pour installation","","","Support pour installation","Support pour installation","Support pour installation","Support pour installation"]
["","Caoutchouc de protection d'orifice","","","Caoutchouc de protection d'orifice","Caoutchouc de protection d'orifice","Caoutchouc de protection d'orifice","Caoutchouc de protection d'orifice"]
["","Douille","","","Douille","Douille","Douille","Douille"]
["","Isolant pour raccord","","","Isolant pour raccord","Isolant pour raccord","Isolant pour raccord","Isolant pour raccord"]
["","Couvercle","","","Couvercle","Couvercle","Couvercle","Couvercle"]
["","Attaches","","","Attaches","Attaches","Attaches","Attaches"]
["","Vis","","","Vis","Vis","Vis","Vis"]
["","Schéma d’installation","","","Schéma d’installation","Schéma d’installation","Schéma d’installation","Schéma d’installation"]
["","Matériau résistant à la rosée","","","Matériau résistant à la rosée","Matériau résistant à la rosée","Matériau résistant à la rosée","Matériau résistant à la rosée"]
["","Câblage de télécommande","","","Câblage de télécommande","Câblage de télécommande","Câblage de télécommande","Câblage de télécommande"]
["Systèmes de commande","Télécommande câblée","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Piping connections","Liquide","DE","mm","9.52","9.52","9.52","9.52"]
["","Gaz","DE","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Puissance absorbée","Rafraîchissement","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Chauffage","Nom.","kW","0.117","0.238","0.238","0.276"]
["Niveau de puissance sonore","Rafraîchissement","","dBA","55","62","63","65"]
["","Chauffage","","dBA","55","62","63","65"]
["Dimensions","Unité","Largeur","mm","600","600","600","600"]
["","","Profondeur","mm","270","350","350","350"]
["","","Hauteur","mm","1,850","1,850","1,850","1,850"]
["Caisson","Colour","","","Blanc frais","Blanc frais","Blanc frais","Blanc frais"]
["Poids","Unité","","kg","39","47","47","47"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Fréquence","","Hz","50/60","50/60","50/60","50/60"]
["","Tension","","V","220-240/220","220-240/220","220-240/220","220-240/220"]