{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":14,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWA-AT"]
[]
[]
[]
[]
["","","","","","FWA01AT","FWA02AT","FWA03AT","FWA04AT","FWA05AT","FWA06AT","FWA07AT","FWA08AT","FWA10AT"]
["Niveau de pression sonore","Très élevé","","","dBA","35","41","45","42","48","52","52","51","54"]
["","Bas","","","dBA","26","25","27","29","34","35","39","36","41"]
["","Haut","","","dBA","33","40","43","41","47","50","51","49","53"]
["Niveau de puissance sonore totale","Très élevé","","","dBA","46","52","56","53","59","63","63","62","65"]
["","Bas","","","dBA","37","36","38","40","45","46","50","47","52"]
["","Haut","","","dBA","44","51","54","52","58","61","62","60","64"]
["Débit d'eau","Rafraîchissement","","Très élevé","l/h","363","456","612","737","906","1,159","1,278","1,455","1,930"]
["","","","Bas","l/h","232","263","320","472","610","776","890","995","1,347"]
["","","","Haut","l/h","342","445","596","705","892","1,109","1,220","1,420","1,892"]
["","Chauffage","","Haut","l/h","342","445","596","705","892","1,109","1,220","1,420","1,892"]
["","","","Très élevé","l/h","363","456","612","737","906","1,159","1,278","1,455","1,930"]
["","","","Bas","l/h","232","263","320","472","610","776","890","995","1,347"]
["","Chute de pression d'eau","Chauffage","Très élevé","kPa","9","14","26","16","25","37","12","15","26"]
["","","","Haut","kPa","8","13","24","14","24","34","11","14","25"]
["","","","Bas","kPa","3","4","6","6","10","15","5","6","12"]
["","","Rafraîchissement","Très élevé","kPa","9","15","29","17","24","43","14","18","33"]
["","","","Haut","kPa","8","14","28","16","24","40","12","17","32"]
["","","","Bas","kPa","4","6","9","8","12","21","7","9","17"]
["Piping connections","Évacuation","","OD","mm","R 3/4\"","R 3/4\"","R 3/4\"","R 3/4\"","R 3/4\"","R 3/4\"","R 3/4\"","R 3/4\"","R 3/4\""]
["","Eau","","Entrée","","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\""]
["","","","Sortie","","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\""]
["Puissance absorbée","Haut","","","kW","0.042","0.059","0.072","0.072","0.105","0.159","0.209","0.219","0.286"]
["","Bas","","","kW","0.04","0.04","0.05","0.05","0.07","0.12","0.17","0.17","0.23"]
["","Super high","","","kW","0.042","0.059","0.073","0.075","0.110","0.163","0.216","0.222","0.288"]
["Dimensions","Unité","","Largeur","mm","590","590","590","590","590","590","590","590","590"]
["","","","Profondeur","mm","705","735","875","1,010","1,010","1,210","1,400","1,560","1,820"]
["","","","Hauteur","mm","253","253","253","253","253","253","253","253","253"]
["Caisson","Colour","","","","Métal","Métal","Métal","Métal","Métal","Métal","Métal","Métal","Métal"]
["Poids","Unité","","","kg","17.0","18.0","21.0","24.0","24.0","30.0","40.0","41.0","47.0"]
["Entrée de courant","Haut","","","A","0.18","0.26","0.32","0.32","0.46","0.70","0.92","0.96","1.26"]
["","Très élevé","","","A","0.18","0.26","0.32","0.33","0.48","0.72","0.95","0.97","1.26"]
["","Bas","","","A","0.16","0.18","0.22","0.24","0.29","0.53","0.74","0.75","1.00"]
["Power supply","Type","","","","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50","50","50","50"]
["","Tension","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]