{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":14,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXFA-A"]
[]
[]
[]
[]
["","","","","","FXFA20A2VEB","FXFA25A2VEB","FXFA32A2VEB","FXFA40A2VEB","FXFA50A2VEB","FXFA63A2VEB","FXFA80A2VEB","FXFA100A2VEB","FXFA125A2VEB"]
["Puissance frigorifique","Puissance totale","","À grande vitesse de ventilation","kW","2.2","2.8","3.6","4.5","5.6","7.1","9.0","11.2","14.0"]
["Puissance calorifique","Puissance totale","","À grande vitesse de ventilation","kW","2.5","3.2","4.0","5.0","6.3","8.0","10.0","12.5","16.0"]
["Puissance absorbée - 50Hz","Rafraîchissement","","À grande vitesse de ventilation","kW","0.017 (1)","0.017 (1)","0.017 (1)","0.018 (1)","0.023 (1)","0.028 (1)","0.045 (1)","0.078 (1)","0.103 (1)"]
["","Chauffage","","À grande vitesse de ventilation","kW","0.017 (1)","0.017 (1)","0.017 (1)","0.018 (1)","0.023 (1)","0.028 (1)","0.045 (1)","0.078 (1)","0.103 (1)"]
["Dimensions","Unité","","Hauteur","mm","204","204","204","204","204","204","246","246","288"]
["","","","Largeur","mm","840","840","840","840","840","840","840","840","840"]
["","","","Profondeur","mm","840","840","840","840","840","840","840","840","840"]
["Poids","Unité","","","kg","18","18","18","19","21","21","24","24","26"]
["Caisson","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Ventilateur","Débit d'air - 50Hz","Rafraîchissement","À grande vitesse de ventilation","m³/min","12.8","12.8","12.8","14.8","15.1","16.6","23.3","28.8","33.0"]
["","","","À petite vitesse de ventilation","m³/min","8.9","8.9","8.9","10.4","10.7","10.7","13.8","13.8","20.6"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Réfrigérant-=-PRP","","","","675","675","675","675","675","675","675","675","675"]
["Niveau de puissance sonore","Rafraîchissement","","À grande vitesse de ventilation","dBA","49.0","49.0","49.0","51.0","51.0","53.0","55.0","60.0","61.0"]
["Niveau de pression sonore","Rafraîchissement","","À grande vitesse de ventilation","dBA","31.0","31.0","31.0","33.0","33.0","35.0","38.0","43.0","45.0"]
["","","","À vitesse moyenne de ventilation","dBA","29.0","29.0","29.0","31.0","31.0","33.0","34.0","37.0","41.0"]
["","","","À petite vitesse de ventilation","dBA","28.0","28.0","28.0","29.0","29.0","30.0","30.0","30.0","36.0"]
["","Chauffage","","À grande vitesse de ventilation","dBA","31.0","31.0","31.0","33.0","33.0","35.0","38.0","43.0","45.0"]
["","","","À vitesse moyenne de ventilation","dBA","29.0","29.0","29.0","31.0","31.0","33.0","34.0","37.0","41.0"]
["","","","À petite vitesse de ventilation","dBA","28.0","28.0","28.0","29.0","29.0","30.0","30.0","30.0","36.0"]
["Raccords de tuyauterie","Liquide","","Type","","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon"]
["","","","DE","mm","6","6","6","6","6","6","6","10","10"]
["","Gaz","","Type","","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon"]
["","","","DE","mm","9.52","9.52","9.52","12.7","12.7","12.7","12.7","15.9","15.9"]
["","Évacuation","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Panneau décoratif","Modèle","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Dimensions","","Hauteur","mm","65","65","65","65","65","65","65","65","65"]
["","","","Largeur","mm","950","950","950","950","950","950","950","950","950"]
["","","","Profondeur","mm","950","950","950","950","950","950","950","950","950"]
["","Poids","","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["Panneau décoratif&nbsp;2","Panneau décoratif&nbsp;2-=-Modèle","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Panneau décoratif&nbsp;2-=-Dimensions","","Panneau décoratif&nbsp;2-=-Dimensions-=-Hauteur-=-mm","mm","148","148","148","148","148","148","148","148","148"]
["","","","Panneau décoratif&nbsp;2-=-Dimensions-=-Largeur-=-mm","mm","950","950","950","950","950","950","950","950","950"]
["","","","Panneau décoratif&nbsp;2-=-Dimensions-=-Profondeur-=-mm","mm","950","950","950","950","950","950","950","950","950"]
["","Panneau décoratif&nbsp;2-=-Poids-=-kg","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["Panneau décoratif&nbsp;3","Panneau décoratif&nbsp;3-=-Modèle","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Panneau décoratif&nbsp;3-=-Dimensions","","Panneau décoratif&nbsp;3-=-Dimensions-=-Hauteur-=-mm","mm","106","106","106","106","106","106","106","106","106"]
["","","","Panneau décoratif&nbsp;3-=-Dimensions-=-Largeur-=-mm","mm","950","950","950","950","950","950","950","950","950"]
["","","","Panneau décoratif&nbsp;3-=-Dimensions-=-Profondeur-=-mm","mm","950","950","950","950","950","950","950","950","950"]
["","Panneau décoratif&nbsp;3-=-Poids-=-kg","","","kg","6.5","6.5","6.5","6.5","6.5","6.5","6.5","6.5","6.5"]
["Filtre à air","Type","","","","Tamis en résine","Tamis en résine","Tamis en résine","Tamis en résine","Tamis en résine","Tamis en résine","Tamis en résine","Tamis en résine","Tamis en résine"]
["Accessoires standard","Washer for hanger bracket","","","","8","8","8","8","8","8","8","8","8"]
["","Wire clamp material","","","","7","7","7","7","7","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2","2","2"]
["","Screws","","","","4","4","4","4","4","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1","1","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Courant&nbsp;- 50&nbsp;Hz","Courant&nbsp;- 50&nbsp;Hz-=-Intensité maximale de fusible (MFA)-=-A","","","A","6","6","6","6","6","6","6","6","6"]
["Remarques","","","","","(1) - Les valeurs sont correctes pour le réglage en usine.","(1) - Les valeurs sont correctes pour le réglage en usine.","(1) - Les valeurs sont correctes pour le réglage en usine.","(1) - Les valeurs sont correctes pour le réglage en usine.","(1) - Les valeurs sont correctes pour le réglage en usine.","(1) - Les valeurs sont correctes pour le réglage en usine.","(1) - Les valeurs sont correctes pour le réglage en usine.","(1) - Les valeurs sont correctes pour le réglage en usine.","(1) - Les valeurs sont correctes pour le réglage en usine."]