{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":102,"n_cols":12,"rows_kept":102,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMA-A"]
[]
[]
[]
[]
["","","","","","FXMA50A5VEB","FXMA63A5VEB","FXMA80A5VEB","FXMA100A5VEB","FXMA125A5VEB","FXMA200AXVMB","FXMA250AXVMB"]
["Niveau de pression sonore","Chauffage","","À grande vitesse de ventilation","dBA","","","","","","48.0"]
["","","","À petite vitesse de ventilation","dBA","","","","","","45.0"]
["","","","À vitesse moyenne de ventilation","dBA","","","","","","46.5"]
["","Rafraîchissement","","À petite vitesse de ventilation","dBA","","","","","","45.0"]
["","","","À grande vitesse de ventilation","dBA","","","","","","48.0"]
["","","","À vitesse moyenne de ventilation","dBA","","","","","","46.5"]
["Accessoires standard","Manuel d'installation et d'exploitation","","","","","","","","","1"]
["","Attache-câble","","","","","","","","","1"]
["","Rondelle à ressort","","","","","","","","","2"]
["","Vis à tête hexagonale","","","","","","","","","2"]
["","Rondelle plate","","","","","","","","","8"]
["","Vis à tête hexagonale avec rondelle","","","","","","","","","49"]
["","Tuyau de raccordement de gaz","","","","","","","","","1"]
["","Précautions générales de sécurité","","","","","","","","","1"]
["Réfrigérant","PRP","","","","","","","","","675"]
["","Type","","","","","","","","","R-32"]
["Puissance absorbée - 50 Hz","Rafraîchissement","","À grande vitesse de ventilation","kW","","","","","","0.54"]
["","Chauffage","","À grande vitesse de ventilation","kW","","","","","","0.54"]
["Puissance frigorifique","Puissance totale","","À grande vitesse de ventilation","kW","","","","","","22.4"]
["","Nom.","","","kW","","","","","","22.4"]
["Piping connections","Liquide","","DE","mm","","","","","","9.5"]
["","","","Type","","","","","","","Raccord à dudgeon"]
["","Gaz","","DE","mm","","","","","","19.1"]
["","","","Type","","","","","","","Bride"]
["","Évacuation","","","","","","","","","BSP1"]
["Niveau de puissance sonore","Rafraîchissement","","À grande vitesse de ventilation","dBA","","","","","","75.0"]
["Dimensions","Unité","","Largeur","mm","","","","","","1,490"]
["","","","Profondeur","mm","","","","","","1,100"]
["","","","Hauteur","mm","","","","","","470"]
["Caisson","Matériau","","","","","","","","","Tôle en acier galvanisé"]
["","Colour","","","","","","","","","Non peint"]
["Poids","Unité","","","kg","","","","","","105"]
["Ventilateur","Pression statique extérieure - 50 Hz","","Haut","Pa","","","","","","250"]
["","","","Bas","Pa","","","","","","50"]
["","Pression statique extérieure - 60 Hz","","Haut","Pa","","","","","","250"]
["","","","Bas","Pa","","","","","","50"]
["","Débit d'air - 50 Hz","Rafraîchissement","À grande vitesse de ventilation","m³/min","","","","","","62"]
["","","","À petite vitesse de ventilation","m³/min","","","","","","41"]
["Puissance calorifique","Puissance totale","","À grande vitesse de ventilation","kW","","","","","","25.0"]
["","Nom.","","","kW","","","","","","25.0"]
["Courant - 50 Hz","Intensité maximale de fusible (MFA)","","","A","","","","","","6"]
["Power supply","Phase","","","","","","","","","1~"]
["","Nom","","","","","","","","","VM"]
["","Fréquence","","","Hz","","","","","","50/60"]
["","Tension","","","V","","","","","","220-240/220-230"]
["Puissance frigorifique","Puissance totale","","À grande vitesse de ventilation","kW","5.6","7.1","9.0","11.2","14.0","","28.0"]
["Puissance calorifique","Puissance totale","","À grande vitesse de ventilation","kW","6.3","8.0","10.0","12.5","16.0","","31.5"]
["Puissance absorbée - 50Hz","Rafraîchissement","","À grande vitesse de ventilation","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["","Chauffage","","À grande vitesse de ventilation","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["Dimensions","Unité","","Hauteur","mm","300","300","300","300","300","","470"]
["","","","Largeur","mm","1,000","1,000","1,000","1,400","1,400","","1,490"]
["","","","Profondeur","mm","700","700","700","700","700","","1,100"]
["Poids","Unité","","","kg","35","35","35","46","46","","115"]
["Caisson","Couleur","","","","Non peint","Non peint","Non peint","Non peint","Non peint","","Non peint"]
["","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","","Tôle en acier galvanisé"]
["Vide de faux-plafond requis >-=-mm","mm","","","","350","350","350","350","350"]
["Ventilateur","Débit d'air - 50Hz","Rafraîchissement","À grande vitesse de ventilation","m³/min","18.0","19.5","25.0","32.0","36.0","","74"]
["","","","À petite vitesse de ventilation","m³/min","15.0","16.0","20.0","23.0","26.0","","52"]
["","Ventilateur-=-Pression statique extérieure - 50&nbsp;Hz","","Ventilateur-=-Pression statique extérieure - 50&nbsp;Hz-=-Haut-=-Pa","Pa","200","200","200","200","200","","250"]
["","Ventilateur-=-Pression statique extérieure - 60&nbsp;Hz","","Ventilateur-=-Pression statique extérieure - 60&nbsp;Hz-=-Haut-=-Pa","Pa","200","200","200","200","200","","250"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32","R-32","","R-32"]
["","Réfrigérant-=-PRP","","","","675","675","675","675","675","","675"]
["Niveau de puissance sonore","Rafraîchissement","","À grande vitesse de ventilation","dBA","61.0","64.0","67.0","65.0","70.0","","76.0"]
["Niveau de pression sonore","Rafraîchissement","","À grande vitesse de ventilation","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","À vitesse moyenne de ventilation","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","À petite vitesse de ventilation","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["","Chauffage","","À grande vitesse de ventilation","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","À vitesse moyenne de ventilation","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","À petite vitesse de ventilation","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["Raccords de tuyauterie","Liquide","","Type","","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","","Raccord à dudgeon"]
["","","","DE","mm","6.35","6.35","6.35","9.52","9.52","","9.5"]
["","Gaz","","Type","","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","Raccord à dudgeon","","Bride"]
["","","","DE","mm","12.7","12.7","12.7","15.9","15.9","","19.1"]
["","Évacuation","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","","BSP1"]
["Filtre à air","Type","","","","Tamis en résine","Tamis en résine","Tamis en résine","Tamis en résine","Tamis en résine"]
["Accessoires standard","Washer for hanger bracket","","","","8","8","8","8","8"]
["","Drain hose","","","","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","","1"]
["","Insulation for fitting","","","","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1"]
["","Screws","","","","16","16","16","16","16"]
["","Sealing pad","","","","3","3","3","3","3"]
["Alimentation électrique","Nom","","","","VE","VE","VE","VE","VE","","VM"]
["","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Fréquence","","","Hz","50/60","50/60","50/60","50/60","50/60","","50/60"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","","220-240/220-230"]
["Courant&nbsp;- 50&nbsp;Hz","Courant&nbsp;- 50&nbsp;Hz-=-Intensité maximale de fusible (MFA)-=-A","","","A","6","6","6","6","6","","6"]
["Ventilateur","Ventilateur-=-Pression statique extérieure - 50&nbsp;Hz","","Ventilateur-=-Pression statique extérieure - 50&nbsp;Hz-=-Bas-=-Pa","Pa","","","","","","","50"]
["","Ventilateur-=-Pression statique extérieure - 60&nbsp;Hz","","Ventilateur-=-Pression statique extérieure - 60&nbsp;Hz-=-Bas-=-Pa","Pa","","","","","","","50"]
["Accessoires standard","General safety precautions","","","","","","","","","","1"]
["","Wire clamp material","","","","","","","","","","1"]
["","Spring washer","","","","","","","","","","2"]
["","Hexagon head screw","","","","","","","","","","2"]
["","Plain washer","","","","","","","","","","8"]
["","Hexagon head screw with washer","","","","","","","","","","49"]
["","Gas connection pipe","","","","","","","","","","1"]