{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL1"]
[]
[]
[]
[]
["","","","","JEHCCU0115CL1","JEHCCU0135CL1"]
["Poids","Unité","","kg","59","61"]
["Dimensions","Unité","Largeur","mm","876","876"]
["","","Profondeur","mm","430","430"]
["","","Hauteur","mm","606","606"]
["Caisson","Couleur","","","Gris clair","Gris clair"]
["Ventilateur","Type","","","Axial","Axial"]
["Power supply","Phase","","","1~","1~"]
["","Fréquence","","Hz","50","50"]
["","Tension","","V","230","230"]
["Remarques","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque"]
["","","","","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés."]