{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":136,"n_cols":14,"rows_kept":136,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHSCU-CL3"]
[]
[]
[]
[]
["","","","","","JEHSCU0300CL3","JEHSCU0400CL3","JEHSCU0500CL3","JEHSCU0600CL3","JEHSCU0750CL3","JEHSCU0951CL3 EVI","JEHSCU0951CL3 EVI_","JEHSCU0200CL3 (Archived)","JEHSCU0950CL3 EVI (Archived)"]
["Puissance frigorifique","Basses températures","R-407F","Nom","kW","","2.38","2.87","","","","","","4.88"]
["Consommation annuelle d'électricité Q","R-407F","","Te -35°C","kWh/a","","10,730.00","13,018.00","","","","","","22,348.00"]
["Paramètres à pleine charge et temp. ext. 43°C","R-407F","Te -35°C","Puissance absorbée (D3)","kW","","3.30"]
["","","","Puissance frigorifique (P3)","kW","","2.04"]
["","","","COP déclaré (COP3)","","","0.62"]
["Poids","Unité","","","kg","78","132","132","133","203","","","76","200"]
["Réfrigérant","PRP","","","","","","","","","","","3,922"]
["","Type","","","","","","","","","","","R-404A"]
["Rapport de performances énergétiques saisonnières SEPR","R-407F","","Te -35°C","","","1.65","1.64","","","","","","1.63"]
["Paramètres à pleine charge et temp. ext. 32°C (Point A)","R-407F","Te -35°C","Puissance absorbée nominale (DA)","kW","","2.51","3.08","","","","","","4.51"]
["","","","COP nominal (COPA)","","","0.95","0.93","","","","","","1.08"]
["","","","Puissance frigorifique nominale (PA)","kW","","2.38","2.87","","","","","","4.88"]
["COP","Low temperature","","R-407F","","","0.95","0.93","","","","","","1.08"]
["Dimensions","Unité","","Largeur","mm","1,101","1,353","1,353","1,353","1,348","","","1,101","1,348"]
["","","","Profondeur","mm","444","575","575","575","605","","","444","605"]
["","","","Hauteur","mm","662","872","872","872","1,727","","","662","1,727"]
["Caisson","Couleur","","","","Gris clair","Gris clair","Gris clair","Gris clair","Gris clair","","","Gris clair","Gris clair"]
["Ventilateur","Type","","","","Axial","Axial","Axial","Axial","Axial","","","Axial","Axial"]
["Power supply","Phase","","","","3~","3~","3~","3~","3~","","","3~","3~"]
["","Fréquence","","","Hz","50","50","50","50","50","","","50","50"]
["","Tension","","","V","400","400","400","400","400","","","400","400"]
["Remarques","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - Se référer à la condition: Temp. ext. = 32°C, temp. d'évap. = -10°C et surchauffe 10K (applic. temp. moy.)"]
["","","","","","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","","","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque"]
["","","","","","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","","","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés."]
["Puissance frigorifique","Basses températures","R-448A","Nom","kW","1.62","2.53","","3.49","4.81"]
["","","R-449A","Nom","kW","1.62","2.53","","3.49","4.81"]
["Paramètres à pleine charge et temp. ext. 43°C","R-449A","Te -35°C","COP déclaré (COP3)","","0.68","0.68","","0.46","0.81"]
["","","","Puissance absorbée (D3)","kW","2.11","3.29","","6.15","5.28"]
["","","","Puissance frigorifique (P3)","kW","1.43","2.23","","2.82","4.26"]
["","R-448A","Te -35°C","Puissance absorbée (D3)","kW","2.11","3.29","","6.15","5.28"]
["","","","COP déclaré (COP3)","","0.68","0.68","","0.46","0.81"]
["","","","Puissance frigorifique (P3)","kW","1.43","2.23","","2.82","4.26"]
["Paramètres à pleine charge et temp. ext. 25°C","R-449A","Te -35°C","COP déclaré (COP2)","","1.16"]
["","","","Puissance absorbée (D2)","kW","1.48"]
["","","","Puissance frigorifique (P2)","kW","1.71"]
["","R-448A","Te -35°C","Puissance frigorifique (P2)","kW","1.71"]
["","","","Puissance absorbée (D2)","kW","1.48"]
["","","","COP déclaré (COP2)","","1.16"]
["Réfrigérant","PRP type 5","","","","1,387","1,387","","1,387","1,387"]
["","Type 5","","","","R-448A","R-448A","","R-448A","R-448A"]
["Paramètres à pleine charge et temp. ext. 32°C (Point A)","R-448A","Te -35°C","Puissance absorbée nominale (DA)","kW","1.67","2.48","","4.19","4.08"]
["","","","COP nominal (COPA)","","0.97","1.02","","0.83","1.18"]
["","","","Puissance frigorifique nominale (PA)","kW","1.62","2.53","","3.49","4.81"]
["","R-449A","Te -35°C","Puissance frigorifique nominale (PA)","kW","1.62","2.53","","3.49","4.81"]
["","","","COP nominal (COPA)","","0.97","1.02","","0.83","1.18"]
["","","","Puissance absorbée nominale (DA)","kW","1.67","2.48","","4.19","4.08"]
["Puissance absorbée","Basses températures","R-448A","Nom","kW","1.67","2.48","","4.19","4.08"]
["","","R-449A","Nom","kW","1.67","2.48","","4.19","4.08"]
["COP","Low temperature","","R-449A","","0.97","1.02","","0.83","1.18"]
["","","","R-448A","","0.97","1.02","","0.83","1.18"]
["Puissance frigorifique","Basses températures","R-407A","Nom.","kW","","2.29","2.77","3.31"]
["Consommation annuelle d'électricité Q","R-407A","","Te -35°C","kWh/a","","10,212.00","12,364.00","15,026.00"]
["","R-449A","","Te -35°C","kWh/a","","11,276.00","","15,878.00","21,856.00"]
["","R-448A","","Te -35°C","kWh/a","","11,276.00","","15,878.00","21,856.00"]
["Paramètres à pleine charge et temp. ext. 43°C","R-407A","Te -35°C","Puiss. frigorifique (P3)","kW","","2.01","2.40","2.88"]
["","","","COP déclaré (COP3)","","","0.67","0.66","0.64"]
["","","","Puissance absorbée (D3)","kW","","2.98","3.64","4.48"]
["Rapport de performances énergétiques saisonnières SEPR","R-448A","","Te -35°C","","","1.67","","1.64","1.64"]
["","R-449A","","Te -35°C","","","1.67","","1.64","1.64"]
["","R-407A","","Te -35°C","","","1.67","1.67","1.64"]
["Réfrigérant","GWP Type 2","","","","","2,107","2,107","2,107"]
["","PRP type 3","","","","","1,825","1,825"]
["","Type 3","","","","","R-407F","R-407F"]
["","Type 2","","","","","R-407A","R-407A","R-407A"]
["Paramètres à pleine charge et temp. ext. 32°C (Point A)","R-407A","Te -35°C","COP nominal (COPA)","","","0.98","0.97","0.93"]
["","","","Puiss. frigorifique nominale (PA)","kW","","2.29","2.77","3.31"]
["","","","Puissance absorbée nominale (DA)","kW","","2.33","2.85","3.57"]
["Puissance absorbée","Basses températures","R-407A","Nom.","kW","","2.33","2.85","3.57"]
["COP","Low temperature","","R-407A","","","0.98","0.97","0.93"]
["Capacité de réfrig.","Temp. basse","R-407A","Nom.","kW","","","","","","4.89","4.89"]
["Puissance frigorifique","Basses températures","R-407F","Nom","kW","","","","","","4.90","4.90"]
["","","R-448A","Nom","kW","","","","","","4.85","4.85"]
["","","R-449A","Nom","kW","","","","","","4.85","4.85"]
["Puiss. absorbée","Temp. basse","R-407A","Nom.","kW","","","","","","4.15","4.15"]
["Puissance absorbée","Basses températures","R-407F","Nom","kW","","","","","","3.86","3.86"]
["","","R-448A","Nom","kW","","","","","","3.95","3.95"]
["","","R-449A","Nom","kW","","","","","","3.95","3.95"]
["COP","Basse température","","R-407A","","","","","","","1.18","1.18"]
["","Basses températures","","R-407F","","","","","","","1.27","1.27"]
["","","","R-448A","","","","","","","1.23","1.23"]
["","","","R-449A","","","","","","","1.23","1.23"]
["Consommation électrique annuelle Q","R-407A","","Te -35°C","kWh/a","","","","","","22108.00","22108.00"]
["Consommation annuelle d'électricité Q","R-407F","","Te -35°C","kWh/a","","","","","","20961.00","20961.00"]
["","R-448A","","Te -35°C","kWh/a","","","","","","21477.00","21477.00"]
["","R-449A","","Te -35°C","kWh/a","","","","","","21477.00","21477.00"]
["Taux de performance énergétique saisonnier SEPR","R-407A","","Te -35°C","","","","","","","1.65","1.65"]
["Rapport de performances énergétiques saisonnières SEPR","R-407F","","Te -35°C","","","","","","","1.74","1.74"]
["","R-448A","","Te -35°C","","","","","","","1.68","1.68"]
["","R-449A","","Te -35°C","","","","","","","1.68","1.68"]
["Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-407A","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-407A-=-Te -35°C","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-407A-=-Te -35°C-=-Puiss. frigorifique nominale (PA)-=-kW","kW","","","","","","4.89","4.89"]
["","","","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-407A-=-Te -35°C-=-Puissance absorbée nominale (DA)-=-kW","kW","","","","","","3.15","3.15"]
["","","","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-407A-=-Te -35°C-=-COP nominal (COPA)","","","","","","","1.18","1.18"]
["Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-407F","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-407F-=-Te -35°C","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-407F-=-Te -35°C-=-Puissance frigorifique nominale (PA)-=-kW","kW","","","","","","4.90","4.90"]
["","","","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-407F-=-Te -35°C-=-Puissance absorbée nominale (DA)-=-kW","kW","","","","","","3.86","3.86"]
["","","","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-407F-=-Te -35°C-=-COP nominal (COPA)","","","","","","","1.27","1.27"]
["","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-448A","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-448A-=-Te -35°C","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-448A-=-Te -35°C-=-Puissance frigorifique nominale (PA)-=-kW","kW","","","","","","4.85","4.85"]
["","","","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-448A-=-Te -35°C-=-Puissance absorbée nominale (DA)-=-kW","kW","","","","","","3.95","3.95"]
["","","","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-448A-=-Te -35°C-=-COP nominal (COPA)","","","","","","","1.23","1.23"]
["","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-449A","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-449A-=-Te -35°C","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-449A-=-Te -35°C-=-Puissance frigorifique nominale (PA)-=-kW","kW","","","","","","4.85","4.85"]
["","","","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-449A-=-Te -35°C-=-Puissance absorbée nominale (DA)-=-kW","kW","","","","","","3.95","3.95"]
["","","","Paramètres à pleine charge et temp. ext. 32&nbsp;°C (Point A)-=-R-449A-=-Te -35°C-=-COP nominal (COPA)","","","","","","","1.23","1.23"]
["Caisson","Couleur","","","","","","","","","Gris clair","Gris clair"]
["Dimensions","Unité","","Hauteur","mm","","","","","","1727","1727"]
["","","","Largeur","mm","","","","","","1348","1348"]
["","","","Profondeur","mm","","","","","","605","605"]
["Poids","Unité","","","kg","","","","","","200","200"]
["Ventilateur","Type","","","","","","","","","Axial","Axial"]
["Réfrigérant","Type 2","","","","","","","","","R-407A","R-407A"]
["","Type 3","","","","","","","","","R-407F","R-407F"]
["","Type 5","","","","","","","","","R-448A","R-448A"]
["","PRP type 2","","","","","","","","","2107","2107"]
["","PRP type 3","","","","","","","","","1825","1825"]
["","PRP type 5","","","","","","","","","1387","1387"]
["Alimentation électrique","Phase","","","","","","","","","3~","3~"]
["","Fréquence","","","Hz","","","","","","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","","","","","400","400"]
["Unité","Courant de fct. nominal (RLA)","R-448A","Rafraîchissement","A","","","","","","8.50","8.50"]
["","","R-449A","Rafraîchissement","A","","","","","","8.50","8.50"]
["Remarques","","","","","","","","","","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque"]
["Consommation électrique annuelle Q","R-404A","","Te -35°C","kWh/a","","","","","","","24503"]
["Taux de performance énergétique saisonnier SEPR","R-404A","","Te -35°C","","","","","","","","1.79"]
["Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-404A","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-404A-=-Te -35°C","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-404A-=-Te -35°C-=-Puiss. frigorifique nominale (PA)-=-kW","kW","","","","","","","5.90"]
["","","","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-404A-=-Te -35°C-=-Puissance absorbée nominale (DA)-=-kW","kW","","","","","","","4.35"]
["","","","Paramètres à pleine charge à temp. ext. 32&nbsp;°C (Point A)-=-R-404A-=-Te -35°C-=-COP nominal (COPA)","","","","","","","","1.36"]
["Paramètres à pleine charge à temp. ext. 43°C","R-404A","Te -35°C","COP déclaré (COP3)","","","","","","","","1.06"]
["Paramètres à pleine charge et temp. ext. 32°C (Point A)","R-404A","Te -35°C","Puiss. frigorifique nominale (PA)","kW","","","","","","","","1.42"]
["","","","Puissance absorbée nominale (DA)","kW","","","","","","","","1.46"]
["","","","COP nominal (COPA)","","","","","","","","","0.97"]
["Paramètres à pleine charge et temp. ext. 25°C","R-404A","Te -35°C","COP déclaré (COP2)","","","","","","","","","1.16"]
["Paramètres à pleine charge et temp. ext. 43°C","R-404A","Te -35°C","COP déclaré (COP3)","","","","","","","","","0.60"]