{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Type","","","","","Purificateur-humidificateur de l'air"]
["Application","","","","","Type console carrossée"]
["Caisson","Couleur","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","700"]
["","","","Largeur","mm","270"]
["","","","Profondeur","mm","270"]
["Poids","Unité","","","kg","9.5"]
["Surface applicable","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Mode purification","Puissance absorbée","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Silence","kW","0.007"]
["Mode humidification","Puissance absorbée","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Silence","kW","0.011"]
["","Mode humidification-=-Capacité du réservoir d'eau-=-L","","","L","2.7"]
["Niveau de pression sonore","Mode purification","","Turbo","dBA","53.0"]
["","","","Moyen","dBA","39.0"]
["","","","Bas","dBA","29.0"]
["","","","Silence","dBA","19.0"]
["","Mode humidification","","Turbo","dBA","53.0"]
["","","","Moyen","dBA","39.0"]
["","","","Bas","dBA","33.0"]
["","","","Silence","dBA","25.0"]
["Ventilateur","Débit d'air","Mode purification","Turbo","m³/h","330"]
["","","","Moyen","m³/h","192"]
["","","","Bas","m³/h","120"]
["","","","Silence","m³/h","54"]
["","","Mode humidification","Turbo","m³/h","330"]
["","","","Moyen","m³/h","192"]
["","","","Bas","m³/h","144"]
["","","","Silence","m³/h","102"]
["Méthode de collecte des poussières","","","","","Filtre HEPA électrostatique"]
["Méthode de désodorisation","","","","","Flash Streamer + catalyseur purificateur"]
["Accessoires standard","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Power cord","Cordon d'alimentation","","","","1.8"]
["Alimentation électrique","Phase","","","","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50/60"]
["","Alimentation électrique-=-Tension","","Alimentation électrique-=-Tension-=-V","","220-240/220-230"]
["Courant de fonctionnement","Mode purification","Courant de fonctionnement-=-Mode purification-=-Turbo","Turbo","","0.50"]
["","","Courant de fonctionnement-=-Mode purification-=-Moyen","Moyen","","0.19"]
["","","Courant de fonctionnement-=-Mode purification-=-Bas","Bas","","0.12"]
["","","Courant de fonctionnement-=-Mode purification-=-Silence","Silence","","0.09"]
["","Mode humidification","Courant de fonctionnement-=-Mode humidification-=-Turbo","Turbo","","0.50"]
["","","Courant de fonctionnement-=-Mode humidification-=-Moyen","Moyen","","0.20"]
["","","Courant de fonctionnement-=-Mode humidification-=-Bas","Bas","","0.15"]
["","","Courant de fonctionnement-=-Mode humidification-=-Silence","Silence","","0.13"]
["Remarques","","","","","(1) - La surface applicable convient pour le fonctionnement de l’unité à la vitesse maximale du ventilateur (HH). La surface applicable fait référence à l'espace dans lequel une certaine quantité de particules de poussière peut être supprimée en 30 minutes. (JEM 1467)"]
["","","","","","(2) - Converti aux normes NRCC depuis les valeurs de test en conformité avec la norme JEM1467."]