{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","NHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","NHY2KOMB28AA","NHY2KOMB32AA"]
["Eau chaude sanitaire","Apport de chaleur (valeur calorifique brute) Qnw","Nom.","Max.","kW","32.3","36.2"]
["","","","Min.","kW","7.9","8.4"]
["","Apport de chaleur (valeur calorifique nette) Qnw","Nom.","Min.","kW","7.2","7.6"]
["","","","Max.","kW","29.1","32.7"]
["","Efficacité","","Nom.","%","105","105"]
["Air d'alimentation","Concentrique","","","","Oui","Oui"]
["Chauffage d'eau chaude sanitaire","Général","","Classe","","A","A"]
["","","","Profil de charge déclaré","","XL","XL"]
["Dimensions","Unité","Hauteur","Caisson","mm","650","710"]
["Caisson","Matériau","","","","Tôle avec précouche","Tôle avec précouche"]
["","Couleur","","","","Blanc - RAL9010","Blanc - RAL9010"]
["Chauffage des locaux","Général","","Classe d'efficacité saisonnière du chauffage de l'air ambiant","","A","A"]
["","","","ηs (efficacité saisonnière du chauffage de l'air ambiant)","%","93","93"]
["Chauff. central","Apport de chaleur Qn (valeur calorifique brute)","Nom.","Min.","kW","8.0","8.3"]
["","","","Max.","kW","26.3","30.0"]
["","Sortie Pn à 80/60°C","","Min.","kW","7.1","7.4"]
["","","","Nom.","kW","23.1","26.6"]
["","Apport de chaleur Qn (valeur calorifique nette)","Nom.","Max.","kW","23.7","27.0"]
["","","","Min.","kW","7.1","7.6"]
["","Sortie Pnc à 50/30°C","","Min.","kW","7.7","8.2"]
["","","","Nom.","kW","25.4","28.9"]
["Gaz","Connexion","","Diamètre","mm","15","15"]
["","Consommation (G31)","","Min.","m³/h","0.28","0.30"]
["","","","Max.","m³/h","1.15","1.29"]
["","Catégorie NOx","","","","6","6"]
["Remarques","","","","","(1) - 80/60","(1) - 80/60"]
["","","","","","(2) - Point de consigne 60 °C","(2) - Point de consigne 60 °C"]
["","","","","","(3) - Point de consigne 40 ℃","(3) - Point de consigne 40 ℃"]