{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":21,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RDV"]
[]
[]
[]
[]
["","","","","","RDV103EA12S3A","RDV103EA12S3B","RDV103EA12S7A","RDV103EA12S7B","RDV105EA12S3A","RDV105EA12S3B","RDV105EA12S7A","RDV105EA12S7B","RDV206EA12S3A","RDV206EA12S3B","RDV206EA12S7A","RDV206EA12S7B","RDV207EA12S3A","RDV207EA12S3B","RDV207EA12S7A","RDV207EA12S7B"]
["Capacité de réfrig.","Temp. moyenne","R-134a","Nom.","kW","0.593","","0.593","","0.912","","0.912","","1.336","","1.336","","1.935","","1.935"]
["Puissance calorifique","R-134a","","Nom","kW","","0.7","","0.9","","1.05","","0.9","","1.4","","1.6","","1.75","","1.6"]
["Caisson","Couleur","","Unité de condensation","","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet","Violet"]
["Dimensions","Unité de condensation","","Largeur","mm","682","","682","","682","","682","","882","","882","","882","","882"]
["","","","Profondeur","mm","337","","337","","337","","337","","427","","427","","427","","427"]
["","Unité d'évaporation","","Hauteur","mm","","570","","215","","570","","215","","570","","215","","570","","215"]
["","","","Largeur","mm","","375","","669","","375","","669","","595","","1089","","595","","1089"]
["","","","Profondeur","mm","","210","","490","","210","","490","","210","","490","","210","","490"]
["Compresseur","Quantité","","","","1","","1","","1","","1","","1","","1","","1","","1"]
["","Type","","","","Par compression de vapeur","","Par compression de vapeur","","Par compression de vapeur","","Par compression de vapeur","","Par compression de vapeur","","Par compression de vapeur","","Par compression de vapeur","","Par compression de vapeur"]
["","Modèle","","","","AE4430Y-FZ1A","","AE4430Y-FZ1A/CSIR","","NEU6212Z/CSI","","NEU6212Z/CSIR","","CAJ4476Y/F/CSIR","","CAJ4476Y/F/CSIR","","CAJ4511Y/F","","CAJ4511Y/F"]
["","Méthode de démarrage","","","","Directe","","Directe","","Directe","","Directe","","Directe","","Directe","","Directe","","Directe"]
["Condenseur","Débit d'air","","","m³/h","600","","600","","1200","","1200","","600","","600","","1100","","1100"]
["Évaporateur","Pulsion d'air","","","m","4","","4","","4","","4","","4","","4","","4","","4"]
["Plage de fonctionnement","Température de chambre froide","","Min.","°C","10","","10","","10","","10","","10","","10","","10","","10"]
["","","","Max.","°C","20","","20","","20","","20","","20","","20","","20","","20"]
["","Température extérieure","","Min.","°C","20","","20","","20","","20","","20","","20","","20","","20"]
["","","","Max.","°C","40","","40","","40","","40","","40","","40","","40","","40"]
["Réfrigérant","","","","","R-134a","","R-134a","","R-134a","","R-134a","","R-134a","","R-134a","","R-134a","","R-134a"]
["","Réfrigérant-=-PRP","","","","1430","","1430","","1430","","1430","","1430","","1430","","1430","","1430"]
["Bouteille de liquide standard","L","","","","1.6","","1.6","","2.5","","2.5","","1.6","","1.6","","2.5","","2.5"]
["Niveau de pression sonore","Nom.","","","dBA","35","","35","","35","","35","","43","","43","","43","","43"]
["Alimentation électrique","Alimentation électrique-=-Tension-=-V","","","V","220-230","","220-230","","220-230","","220-230","","220-230","","220-230","","220-230","","220-230"]
["","Phase","","","","1~","","1~","","1~","","1~","","1~","","1~","","1~","","1~"]
["","Fréquence","","","Hz","50","","50","","50","","50","","50","","50","","50","","50"]