{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B2V1B","RXA42B5V1B","RXA50B2V1B","RXA50B5V1B"]
["Dimensions","Unité","","Hauteur","mm","734","","734","734"]
["","","","Largeur","mm","870","","870","954"]
["","","","Profondeur","mm","373","","373","401"]
["Poids","Unité","","","kg","50","","50","49"]
["Compresseur","Type","","","","Compresseur swing hermétique","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","","-10","-10"]
["","","","Max.","°CBS","46","","46","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","","-15","-15"]
["","","","Max.","°CBH","18","","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","48.0","","48.0","48"]
["","Chauffage","","Nom.","dBA","48.0","","48.0","48"]
["Réfrigérant","","","","","R-32","","R-32","R-32"]
["","Charge","","","kg","1.10","","1.10","1.1"]
["","Réfrigérant-=-Charge-=-Téq. CO₂","","","Téq. CO₂","0.75","","0.75","0.75"]
["","Réfrigérant-=-PRP","","","","675","","675","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","30","","30","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","20","","20","20"]
["Accessoires standard","Installation manual","","","","1","","1","1"]
["","Étiquette de charge de réfrigérant","","","","1","","1","1"]
["","Étiquettes multilingues de gaz à effet de serre fluorés","","","","1","","1","1"]
["","Drain cap","","","","3","","3","3"]
["","Drain plug","","","","1","","1","1"]
["Classe d'efficacité énergétique","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Alimentation électrique","Phase","","","","1~","","1~","1~"]
["","Fréquence","","","Hz","50","","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","","220-240","220-240"]
["Remarques","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement","","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(2) - Pour les données électriques, se reporter au schéma séparé.","","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","","(3) - Contient des gaz à effet de serre fluorés.","","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés."]