{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXB-B"]
[]
[]
[]
[]
["","","","","","RXB25B5V1","RXB25B6V1","RXB25B6V19","RXB35B5V1","RXB35B6V1","RXB35B6V19","RXB50BV1B","RXB60BV1B"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","","","","","","","51","51"]
["","Rafraîchissement","","Nom.","dBA","","","","","","","51","51"]
["Réfrigérant","Charge","","","TCO2Eq","","","","","","","3","3"]
["","PRP","","","","","","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","","","","","","1.45","1.45"]
["","Type","","","","","","","","","","R-410A","R-410A"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Max.","°CBS","","","","","","","46","46"]
["","","","Min.","°CBS","","","","","","","-10","-10"]
["","Chauffage","Extérieure","Max.","°CBH","","","","","","","18","18"]
["","","","Min.","°CBH","","","","","","","-15","-15"]
["Compresseur","Type","","","","","","","","","","Swing hermétique","Swing hermétique"]
["Dimensions","Unité","","Largeur","mm","","","","","","","855","855"]
["","","","Profondeur","mm","","","","","","","328","328"]
["","","","Hauteur","mm","","","","","","","753","753"]
["Poids","Unité","","","kg","","","","","","","44","44"]
["Power supply","Phase","","","","","","","","","","1~","1~"]
["","Fréquence","","","Hz","","","","","","","50","50"]
["","Tension","","","V","","","","","","","220-240","220-240"]
["Remarques","","","","","","","","","","","(1) - Toutes les unités sont testées et conformes à la norme ISO5151 (unité non gainée) ou ISO13253 (unité gainée)","(1) - Toutes les unités sont testées et conformes à la norme ISO5151 (unité non gainée) ou ISO13253 (unité gainée)"]
["","","","","","","","","","","","(2) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis.","(2) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis."]
["","","","","","","","","","","","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","550","550","550","550","550","550"]
["","","","Largeur","mm","658","658","658","658","658","658"]
["","","","Profondeur","mm","275","275","275","275","275","275"]
["Poids","Unité","","","kg","27","26","26","29","28","28"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46","46","46","48","48","48"]
["","Chauffage","","Haut","dBA","47","47","47","48","48","48"]
["Réfrigérant","","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Charge","","","kg","0.74","0.74","0.74","1.00","1.00","1.00"]
["","Charge","","","tCO2Eq","1.5","1.5","1.5","2.1","2.1","2.1"]
["","Réfrigérant-=-PRP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","15","15","15","15","15","15"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","12","12","12","12","12","12"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","","-10","-10","","-10","-10"]
["","","","Max.","°CBS","","46","46","","46","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","","-15","-15","","-15","-15"]
["","","","Max.","°CBH","","18","18","","18","18"]