{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-D"]
[]
[]
[]
[]
["","","","","","RXF20D5V1B","RXF25D5V1B","RXF35D5V1B","RXF42D5V1B","RXF50D5V1B","RXF50D6V1B","RXF60D5V1B","RXF71D5V1B"]
["Dimensions","Unité","","Hauteur","mm","550","550","550","550","734","734","734","734"]
["","","","Largeur","mm","658","658","658","658","870","870","870","870"]
["","","","Profondeur","mm","275","275","275","275","373","373","373","373"]
["Poids","Unité","","","kg","24.0","24.0","24.0","28.0","46","46","50","50"]
["Compressor","Type","","","","","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CBS","48","48","48","48","48","48","48","48"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","-15","-15","-15","-15","-10","-15","-15"]
["","","","Max.","°CBH","18","18","18","18","18","18","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46.0","46.0","48.0","48.0"]
["","","","Nom.","dBA","","","","","47","47","49","52"]
["","Chauffage","","Haut","dBA","47.0","47.0","48.0","48.0"]
["","","","Nom.","dBA","","","","","49","49","49","52"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","0.450","0.450","0.550","0.750","0.9","0.9","1.15","1.15"]
["","Charge","","","tCO2Eq","0.300","0.300","0.370","0.510","0.61","0.61","0.78","0.78"]
["","Réfrigérant-=-PRP","","","","675.0","675.0","675.0","675.0","675","675","675","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20","20","20","20","30","30","30","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","12.0","12.0","12.0","12.0","20","20","20","20"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain cap","","","","","","","","3","3","3","3"]
["","Drain plug","","","","1","1","1","1","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Remarques","","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés."]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Accessoires standard","General safety precautions","","","","1","1","1","1"]