{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","47","48"]
["","Rafraîchissement","","Haut","dBA","","46","48"]
["Accessoires standard","Joint (évacuation)","","","","","1","1"]
["","Manuel d'installation","","","","","1","1"]
["Réfrigérant","Charge","","","TCO2Eq","","2.2","2.2"]
["","PRP","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","1.05","1.05"]
["","Type","","","","","R-410A","R-410A"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","","780","780"]
["","","Chauffage","Très lent","tr/min","","740","740"]
["Raccords de tuyauterie","Dénivelé","UI - UE","Max.","m","","15","15"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["Compresseur","Type","","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","","765","765"]
["","","","Profondeur","mm","","285","285"]
["","","","Hauteur","mm","","550","550"]
["Poids","Unité","","","kg","","35","35"]
["Ventilateur","Débit d’air","Chauffage","Très lent","cfm","","932","932"]
["","","Rafraîchissement","Extra lent","cfm","","1,094","1,094"]
["Power supply","Phase","","","","","1~","1~"]
["","Fréquence","","","Hz","","50","50"]
["","Tension","","","V","","220-240","220-240"]
["Remarques","","","","","(1) - 220V","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 230 V","(3) - 230 V","(3) - 240V"]
["","","","","","(4) - Plage de fonctionnement en combinaison avec Nexura, FVXG-K, rafraîchissement : 10 °CBS min. ~ 46 °CBS max.; chauffage : -15 °CBH min. ~ 18 °CBH max.","(4) - 240V","(4) - 240V","(4) - Plage de fonctionnement en combinaison avec Nexura, FVXG-K, rafraîchissement : 10 °CBS min. ~ 46 °CBS max.; chauffage : -15 °CBH min. ~ 18 °CBH max."]
["","","","","","","(5) - Plage de fonctionnement en combinaison avec Nexura, FVXG-K, rafraîchissement : 10 °CBS min. ~ 46 °CBS max.; chauffage : -15 °CBH min. ~ 18 °CBH max.","(5) - Plage de fonctionnement en combinaison avec Nexura, FVXG-K, rafraîchissement : 10 °CBS min. ~ 46 °CBS max.; chauffage : -15 °CBH min. ~ 18 °CBH max."]
["","","","","","","(6) - Contient des gaz à effet de serre fluorés.","(6) - Contient des gaz à effet de serre fluorés."]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","m³/min","31.0","","","42.6"]
["","","Chauffage","Très lent","m³/min","26.4","","","38.3"]
["","","","Extra lent","cfm","1094","","","1504"]
["","","Chauffage","Très lent","cfm","932","","","1352"]
["Dimensions","Unité","","Hauteur","mm","550","","","735"]
["","","","Largeur","mm","765","","","825"]
["","","","Profondeur","mm","285","","","300"]
["Poids","Unité","","","kg","35","","","48"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","780","","","670"]
["","","Chauffage","Très lent","tr/min","740","","","670"]
["Compresseur","Type","","","","Compresseur swing hermétique","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10 (5)","","","-10 (5)"]
["","","","Max.","°CBS","46","","","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","","","-15"]
["","","","Max.","°CBH","18","","","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46","","","48"]
["","Chauffage","","Haut","dBA","47","","","48"]
["Réfrigérant","","","","","R-410A","","","R-410A"]
["","Charge","","","kg","1.05","","","1.6"]
["","Charge","","","tCO2Eq","2.2","","","3.3"]
["","Réfrigérant-=-PRP","","","","2087.5","","","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20","","","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","","","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","15","","","20"]
["Accessoires standard","Installation manual","","","","1","","","1"]
["","Joint (drain)","","","","1","","","1"]
["Alimentation électrique","Phase","","","","1~","","","1~"]
["","Fréquence","","","Hz","50","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","","","220-240"]