{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","m³/min","30.6","30.6"]
["","","Chauffage","Très lent","m³/min","27.2","27.2"]
["","","","Extra lent","cfm","1080","1080"]
["","","Chauffage","Très lent","cfm","960","960"]
["Dimensions","Unité","","Hauteur","mm","550","550"]
["","","","Largeur","mm","858","858"]
["","","","Profondeur","mm","330","330"]
["Poids","Unité","","","kg","40","40"]
["Compresseur","Type","","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","46","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-25","-25"]
["","","","Max.","°CBH","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","48","48"]
["","","","Bas","dBA","44","44"]
["","Chauffage","","Haut","dBA","49","49"]
["","","","Bas","dBA","45","45"]
["Réfrigérant","","","","","R-410A","R-410A"]
["","Charge","","","kg","1","1"]
["","Charge","","","tCO2Eq","2.1","2.1"]
["","Réfrigérant-=-PRP","","","","2087.5","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UI","Max.","m","15","15"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]
["Compresseur","Type","","","","Compresseur swing hermétique"]