{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTA-B"]
[]
[]
[]
[]
["","","","","","RXTA30B2V1B"]
["Dimensions","Unité","","Hauteur","mm","551"]
["","","","Largeur","mm","763"]
["","","","Profondeur","mm","312"]
["Poids","Unité","","","kg","38"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","450"]
["","","Chauffage","Très lent","tr/min","360"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10"]
["","","","Max.","°CBS","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-25"]
["","","","Max.","°CBH","18"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","48"]
["","Chauffage","","Nom.","dBA","49"]
["Réfrigérant","","","","","R-32"]
["","Charge","","","kg","1.1"]
["","Charge","","","tCO2Eq","0.74"]
["","Réfrigérant-=-PRP","","","","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","15"]
["Accessoires standard","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240"]