{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N9"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B9","RXTP35N2V1B9"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","49","49"]
["","Rafraîchissement","","Nom.","dBA","48","48"]
["Accessoires standard","Manuel d'installation","","","","1","1"]
["","Étiquette de charge de réfrigérant","","","","1","1"]
["","Étiquettes multilingues de gaz à effet de serre fluorés","","","","1","1"]
["Réfrigérant","Charge","","","TCO2Eq","0.75","0.75"]
["","PRP","","","","675","675"]
["","Charge","","","kg","1.1","1.1"]
["","Type","","","","R-32","R-32"]
["Moteur de ventil.","Vitesse","Rafraîchissement","Extra lent","tr/min","450","450"]
["","","Chauffage","Très lent","tr/min","360","360"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Max.","°CBS","46","46"]
["","","","Min.","°CBS","-10","-10"]
["","Chauffage","Extérieure","Max.","°CBH","18","18"]
["","","","Min.","°CBH","-25","-25"]
["Raccordements de tuyauterie","Dénivelé","UI - UE","Max.","m","15","15"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","763","763"]
["","","","Profondeur","mm","312","312"]
["","","","Hauteur","mm","551","551"]
["Poids","Unité","","","kg","38","38"]
["Power supply","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","220-240","220-240"]
["Remarques","","","","","(1) - Contient des gaz à effet de serre fluorés.","(1) - Contient des gaz à effet de serre fluorés."]
["","","","","","(2) - Voir le schéma séparé pour la plage de fonctionnement","(2) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(3) - Pour les données électriques, se reporter au schéma séparé.","(3) - Pour les données électriques, se reporter au schéma séparé."]