{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":9,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXV-AB"]
[]
[]
[]
[]
["","","","","","RXV25AV1B","RXV35AV1B","RXV50AV1B","RXV60AV1B"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","","","","58"]
["Réfrigérant","Charge","","","TCO2Eq","","","","4.3"]
["","PRP","","","","","","","2,087.5"]
["","Charge","","","kg","","","","2.05"]
["","Type","","","","","","","R-410A"]
["Piping connections","Dénivelé","UI - UE","Max.","m","","","","10"]
["Dimensions","Unité","","Largeur","mm","","","","980"]
["","","","Profondeur","mm","","","","427"]
["","","","Hauteur","mm","","","","790"]
["Poids","Unité","","","kg","","","","60"]
["Remarques","","","","","","","","(1) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","540","540","700"]
["","","","Largeur","mm","776","776","955"]
["","","","Profondeur","mm","320","320","396"]
["Poids","Unité","","","kg","28","29","45"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","18","18","18"]
["","","","Max.","°CBS","43","43","43"]
["","Chauffage","Temp. ext.","Min.","°CBH","-10","-10","-10"]
["","","","Max.","°CBH","24","24","24"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","51","53","56"]
["Réfrigérant","","","","","R-410A","R-410A","R-410A"]
["","Charge","","","kg","0.80","0.95","1.45"]
["","Charge","","","tCO2Eq","1.7","2","3"]
["","Réfrigérant-=-PRP","","","","2087.5","2087.5","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","15","15","25"]
["","Dénivelé","UI - UE","Max.","m","10","10","10"]