{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NY1"]
[]
[]
[]
[]
["","","","","","RZAG71N2Y1B","RZAG71N7Y1B","RZAG100N7Y1B","RZAG100N2Y1B","RZAG125N2Y1B","RZAG125N7Y1B","RZAG140N7Y1B","RZAG140N2Y1B"]
["Dimensions","Unité","","Hauteur","mm","870","870","870","870","870","870","870","870"]
["","","","Largeur","mm","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","Profondeur","mm","460","460","460","460","460","460","460","460"]
["Poids","Unité","","","kg","81","81","85","85","94","94","94","94"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Max.","°CBS","52","52","52","52","52","52","52","52"]
["","Chauffage","Temp. ext.","Min.","°CWB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Max.","°CWB","18","18","18","18","18","18","18","18"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","64","64","66","66","69","69","70","70"]
["","Chauffage","","","dBA","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","46","46","47","47","49","49","50","50"]
["","Chauffage","","Nom.","dBA","48","48","50","50","52","52","52","52"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","3.20","3.2","3.2","3.20","3.70","3.7","3.7","3.70"]
["","Réfrigérant-=-PRP","","","","675","675","675","675","675","675","675","675"]
["","Charge","","","tCO2Eq","2.16","2.16","2.16","2.16","2.50","","2.5","2.50"]
["Raccords de tuyauterie","Liquide","","DE","mm","10","10","10","10","10","10","10","10"]
["","Gaz","","DE","mm","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["","Longueur de tuyauterie","Max.","UE - UI","m","55","55","85","85","85","85","85","85"]
["","","Système","Équivalente","m","75","75","100","100","100","100","100","100"]
["","","","Préchargé d'usine jusqu'à","m","40","40","40","40","40","40","40","40"]
["","Charge de réfrigérant supplémentaire","","","kg/m","Voir le manuel d'installation","Voir le manuel d'installation","Voir le manuel d'installation","Voir le manuel d'installation","Voir le manuel d'installation","Voir le manuel d'installation","Voir le manuel d'installation","Voir le manuel d'installation"]
["","Dénivelé","UI - UE","Max.","m","30","30","30","30","30","30","30","30"]
["","","UI - UI","Max.","m","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["Alimentation électrique","Phase","","","","3~","3~","3~","3~","3~","3~","3~","3~"]
["","Fréquence","","","Hz","50","50","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","380-415","380-415","380-415","380-415","380-415","380-415","380-415","380-415"]
["Courant&nbsp;- 50&nbsp;Hz","Courant&nbsp;- 50&nbsp;Hz-=-Intensité maximale de fusible (MFA)-=-A","","","A","16","16","16","16","16","","16","16"]
["Remarques","","","","","","","","","(1) - Conforme à la norme ENER Lot 21","(1) - Conforme à la norme ENER Lot 21","(1) - Conforme à la norme ENER Lot 21","(1) - Conforme à la norme ENER Lot 21"]
["Réfrigérant","Réfrigérant-=-Charge-=-Téq. CO₂","","","Téq. CO₂","","","","","","2.5"]
["Courant - 50 Hz","Courant - 50 Hz-=-Intensité maximale de fusible (MFA)-=-A","","","A","","","","","","16"]