{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQG-LV1L"]
[]
[]
[]
[]
["","","","","","RZQG71L9V1L"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","64"]
["Dimensions","Unité","","Hauteur","mm","990"]
["","","","Largeur","mm","940"]
["","","","Profondeur","mm","320"]
["Poids","Unité","","","kg","69.0"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-15"]
["","","","Max.","°CBS","50"]
["","Chauffage","Temp. ext.","Min.","°CBH","-20"]
["","","","Max.","°CBH","16"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","48"]
["","Chauffage","","Nom.","dBA","50"]
["","Mode Nuit","","Niveau 1","dBA","43"]
["Réfrigérant","Charge","","","kg","2.9"]
["","Charge","","","tCO2Eq","6.10"]
["","Réfrigérant-=-PRP","","","","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","50"]
["","Dénivelé","UI - UE","Max.","m","30.0"]
["","","UI - UI","Max.","m","0.5"]
["Accessoires standard","Installation manual","","","","1"]
["","Tie-wraps","","","","2"]
["Alimentation électrique","Fréquence","","","Hz","50"]
["Remarques","","","","","(1) - 3 with re-charging"]