{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLCO2"]
[]
[]
[]
[]
["","","","","WLCO2."]
["Nombre maximum d'unités intérieures connectables","","","","0"]
["Nombre maximum d'unités extérieures connectables","","","","0"]
["Caisson","Couleur","","","Blanc"]
["","Couvercle de boutons","","","Non"]
["","DEL de fonctionnement","Couleur","","Vert"]
["Dimensions","Unité","Hauteur","mm","95"]
["","","Largeur","mm","95.0"]
["","","Profondeur","mm","62.0"]
["","Unité emballée","Hauteur","mm","565"]
["","","Largeur","mm","375"]
["","","Profondeur","mm","280"]
["Poids","Unité","","kg","0.126"]
["Emballage","Matériau","","","Carton"]
["","Poids","","kg","0.046"]
["Température extérieure","Fonctionnement","Min.","°C","-10"]
["","","Max.","°C","50"]
["","Stockage","Min.","°C","-20"]
["","","Max.","°C","60"]
["","Température extérieure-=-Humidité relative <-=-%","","%","90"]
["Installation","","","","Installation intérieure"]