{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B","2MXS40H3V1B2","2MXS40H2V1B","2MXS50H3V1B","2MXS50H3V1B2","2MXS50H2V1B"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","48","48","","50","50"]
["","Raffrescamento","","Nom.","dBA","47","47","","48","48"]
["Accessori standard","Manuale di installazione","","","","1","1","","1","1"]
["","Sacchetto viti","","","","1","1","","1","1"]
["","Tappo di scarico","","","","1","1","","1","1"]
["","Gruppo riduttore","","","","","","","1","1"]
["Refrigerante","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Carica","","","kg","1.20","1.20","","1.60","1.60"]
["","Tipo","","","","R-410A","R-410A","","R-410A","R-410A"]
["Piping connections","Dislivello","int. - int.","Max.","m","7.5","7.5","","7.5","7.5"]
["","","int. - est.","Max.","m","15","15","","15","15"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 20m)","0,02 (per lunghezza delle tubazioni superiore ai 20m)","","0,02 (per lunghezza delle tubazioni superiore ai 20m)","0,02 (per lunghezza delle tubazioni superiore ai 20m)"]
["","Lunghezza totale delle tubazioni","Sistema","Reale","m","30","30","","30","30"]
["Compressore","Type","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Dimensioni","Unità","","Larghezza","mm","765","765","","765","765"]
["","","","Profondità","mm","285","285","","285","285"]
["","","","Altezza","mm","550","550","","550","550"]
["Peso","Unità","","","kg","38","38","","42","42"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Frequenza","","","Hz","50","50","","50","50"]
["","Tensione","","","V","220-240","220-240","","220-240","220-240"]
["Note","","","","","(1) - Contiene gas fluorurati a effetto serra","(1) - Contiene gas fluorurati a effetto serra","","(1) - Contiene gas fluorurati a effetto serra","(1) - Contiene gas fluorurati a effetto serra"]
["Dimensioni","Unità","","Altezza","mm","","","550","","","550"]
["","","","Larghezza","mm","","","765","","","765"]
["","","","Profondità","mm","","","285","","","285"]
["Peso","Unità","","","kg","","","38","","","42"]
["Compressore","Type","","","","","","Compressore ermetico tipo Swing","","","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","","","10","","","10"]
["","","","Max.","°CBS","","","46","","","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","","","-15","","","-15"]
["","","","Max.","°CBU","","","15.5","","","15.5"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","","","47","","","48"]
["","Riscaldamento","","Nom.","dBA","","","48","","","50"]
["Refrigerante","Tipo","","","","","","R-410A","","","R-410A"]
["","Carica","","","kg","","","1.20","","","1.60"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","","20","","","20"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","","0,02 (per lunghezza delle tubazioni superiore ai 20m)","","","0,02 (per lunghezza delle tubazioni superiore ai 20m)"]
["","Dislivello","int. - est.","Max.","m","","","15","","","15"]
["","","int. - int.","Max.","m","","","7.5","","","7.5"]
["Attacchi tubazioni","Lunghezza totale delle tubazioni","Sistema","Reale","m","","","30","","","30"]
["Accessori standard","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Alimentazione","Fase","","","","","","1~","","","1~"]
["","Frequenza","","","Hz","","","50","","","50"]
["","Tensione","","","V","","","220-240","","","220-240"]
["Accessori standard","Reducer assembly","","","","","","","","","1"]