{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","47"]
["","Raffrescamento","","Nom.","dBA","46"]
["Accessori standard","Manuale di installazione","","","","1"]
["","Sacchetto viti","","","","1"]
["","Tappo di scarico","","","","1"]
["","Tappo di scarico (1)","","","","6"]
["","Tappo di scarico (2)","","","","3"]
["","Rimuovere l’etichetta F-gas","","","","1"]
["","Etichetta carica di refrigerante","","","","1"]
["Refrigerante","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Carica","","","kg","1.8"]
["","Tipo","","","","R-32"]
["Motore ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","420"]
["","","Riscaldamento","Bassissimo","giri/min","420"]
["Attacchi tubazioni","Dislivello","int. - int.","Max.","m","7.5"]
["","","int. - est.","Max.","m","15"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 30m)"]
["","Lunghezza totale delle tubazioni","Sistema","Reale","m","50"]
["Compressor","Type","","","","Compressore ermetico tipo Swing"]
["Dimensioni","Unità","","Larghezza","mm","868"]
["","","","Profondità","mm","320"]
["","","","Altezza","mm","734"]
["Peso","Unità","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Frequenza","","","Hz","50"]
["","Tensione","","","V","220-240"]
["Note","","","","","(1) - Contiene gas fluorurati a effetto serra"]
["","","","","","(2) - Per informazioni sul campo di funzionamento consultare i disegni separati"]
["","","","","","(3) - Consultare i disegni separati per i dati elettrici"]
["Ventilatore","Portata d'aria","Raffrescamento","Bassissimo","m³/min","","24"]
["","","Riscaldamento","Bassissimo","m³/min","","24"]
["","","","Bassissimo","cfm","","847"]
["","","Riscaldamento","Bassissimo","cfm","","847"]
["Dimensioni","Unità","","Altezza","mm","","734"]
["","","","Larghezza","mm","","868"]
["","","","Profondità","mm","","320"]
["Peso","Unità","","","kg","","57"]
["Motore del ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","","420"]
["","","Riscaldamento","Bassissimo","giri/min","","420"]
["Compressor","Type","","","","","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","","-10"]
["","","","Max.","°CBS","","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","","-15"]
["","","","Max.","°CBU","","18"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","","46"]
["","Riscaldamento","","Nom.","dBA","","47"]
["Refrigerante","Tipo","","","","","R-32"]
["","Carica","","","kg","","1.80"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","25"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","0,02 (per lunghezza delle tubazioni superiore ai 30m)"]
["","Dislivello","int. - est.","Max.","m","","15"]
["","","int. - int.","Max.","m","","7.5"]
["Attacchi tubazioni","Lunghezza totale delle tubazioni","Sistema","Reale","m","","50"]
["Accessori standard","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Alimentazione","Fase","","","","","1~"]
["","Frequenza","","","Hz","","50"]
["","Tensione","","","V","","220-240"]