{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B","3MXM52N2V1B","3MXM68N2V1B"]
["Ventilatore","Portata d'aria","Raffrescamento","Bassissimo","m³;/min","24","24","24.1"]
["","","Riscaldamento","Bassissimo","m³;/min","24","24","24.1"]
["","","","Bassissimo","cfm","847","847","851"]
["","","Riscaldamento","Bassissimo","cfm","847","847","851"]
["Dimensioni","Unità","","Altezza","mm","734","734","734"]
["","","","Larghezza","mm","958","958","958"]
["","","","Profondità","mm","340","340","340"]
["Peso","Unità","","","kg","57","57","62"]
["Motore del ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","420","420"]
["","","Riscaldamento","Bassissimo","giri/min","420","420"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10","-10","-10"]
["","","","Max.","°CBS","46","46","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","-15","-15","-15"]
["","","","Max.","°CBU","18","18","18"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","46","46","48"]
["","Riscaldamento","","Nom.","dBA","47","47","48"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32"]
["","Carica","","","kg","1.80","1.80","2.00"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","1.2","1.2","1.4"]
["","GWP","","","","675","675","675"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","25","25","25"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 30m)","0,02 (per lunghezza delle tubazioni superiore ai 30m)","0,02 (per lunghezza delle tubazioni superiore ai 30m)"]
["","Dislivello","int. - est.","Max.","m","15","15","15"]
["","","int. - int.","Max.","m","7.5","7.5","7.5"]
["Attacchi tubazioni","Lunghezza totale delle tubazioni","Sistema","Reale","m","50","50","50"]
["Accessori standard","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Alimentazione","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240"]
["Accessori standard","Drain cap","","","","","","3"]
["","Reducer assembly","","","","","","1"]