{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Dimensioni","Unità","","Altezza","mm","734","734"]
["","","","Larghezza","mm","1040","1040"]
["","","","Profondità","mm","408","408"]
["Peso","Unità","","","kg","69","73"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","46","46"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","48","52"]
["","Riscaldamento","","Nom.","dBA","49","53"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carica","","","kg","2","2.4"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","25 (2)","25 (3)"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 30m)","0,02 (per lunghezza delle tubazioni superiore ai 30m)"]
["","Dislivello","int. - est.","Max.","m","15 (3)","15"]
["","","int. - int.","Max.","m","7.5 (3)","7.5 (3)"]
["Attacchi tubazioni","Lunghezza totale delle tubazioni","Sistema","Reale","m","60","75"]
["Accessori standard","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Intervallo di efficienza energetica","","","","","A+++ ~ D","A+++ ~ D"]
["Alimentazione","Fase","","","","1~","1~"]
["","Frequenza","","","Hz","50","50"]
["","Tensione","","","V","220-440","220-240"]
["Note","","","","","(1) - Per informazioni sul campo di funzionamento consultare i disegni separati","(1) - Per informazioni sul campo di funzionamento consultare i disegni separati"]
["","","","","","(2) - Per un locale","(2) - Per un locale"]
["","","","","","(3) - Per un locale (per la combinazione con FBA71/100/125 e EKHWET e CKHWS, consultare il manuale di installazione)","(3) - Per un locale (per la combinazione con FBA71/100/125 e EKHWET e CKHWS, consultare il manuale di installazione)"]
["","","","","","(4) - Contiene gas fluorurati a effetto serra","(4) - Contiene gas fluorurati a effetto serra"]