{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXB-C"]
[]
[]
[]
[]
["","","","","","ARXB25C2V1B","ARXB25C5V1B9","ARXB35C2V1B","ARXB35C5V1B9","ARXB50CV1B","ARXB60CV1B"]
["Livello pressione sonora","Riscaldamento","","Nom.","dBA","","","","","51"]
["","Raffrescamento","","Nom.","dBA","","","","","51"]
["Refrigerante","Charge","","","TCO2Eq","","","","","3.0"]
["","GWP","","","","","","","","2,087.5"]
["","Carica","","","kg","","","","","1.45"]
["","Tipo","","","","","","","","R-410A"]
["Compressore","Tipo","","","","","","","","Swing ermetico"]
["Dimensioni","Unità","","Larghezza","mm","","","","","855"]
["","","","Profondità","mm","","","","","328"]
["","","","Altezza","mm","","","","","753"]
["Peso","Unità","","","kg","","","","","44"]
["Power supply","Fase","","","","","","","","1~"]
["","Frequenza","","","Hz","","","","","50"]
["","Tensione","","","V","","","","","220-240"]
["Note","","","","","","","","","(1) - Contiene gas fluorurati a effetto serra"]
["Dimensioni","Unità","","Altezza","mm","550","550","550","550","","753"]
["","","","Larghezza","mm","658","658","658","658","","855"]
["","","","Profondità","mm","275","275","275","275","","328"]
["Peso","Unità","","","kg","28","26","30","28","","44"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","","Swing ermetico"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10","-10","-10","-10","","-10"]
["","","","Max.","°CBS","46","46","46","46","","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","-15","-15","-15","-15","","-15"]
["","","","Max.","°CBU","18","18","18","18","","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","46","46","48","48"]
["","Riscaldamento","","Alta","dBA","47","47","48","48"]
["Refrigerante","Tipo","","","","R-410A","R-410A","R-410A","R-410A","","R-410A"]
["","Carica","","","kg","0.74","0.74","1.0","1.0","","1.45"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","1.5","1.5","2.1","2.1","","3.0"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","","2087.5"]
["Accessori standard","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1"]
["Alimentazione","Fase","","","","1~","1~","1~","1~","","1~"]
["","Frequenza","","","Hz","50","50","50","50","","50"]
["","Tensione","","","V","220-240","220-240","220-240","220-240","","220-240"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","15","","15","","30"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","0,02 (per lunghezza delle tubazioni superiore ai 10m)","","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["Accessori standard","LOT10 Energy Label","","","","","LOT10 Energy Label","","LOT10 Energy Label"]
["Livello pressione sonora","Raffrescamento","","Nom.","dBA","","","","","","51"]
["","Riscaldamento","","Nom.","dBA","","","","","","51"]