{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-M"]
[]
[]
[]
[]
["","","","","","ARXM25M2V1B","ARXM35M2V1B","ARXM50MV1B"]
["Dimensioni","Unità","","Altezza","mm","550","550","735"]
["","","","Larghezza","mm","765","765","825"]
["","","","Profondità","mm","285","285","300"]
["Peso","Unità","","","kg","32","32","44"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","-10","-10","-10"]
["","","","Max.","°CBS","46","46","46"]
["","Riscaldamento","T. esterna","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","46","49","48"]
["","","","Bassa","dBA","","","44"]
["","Riscaldamento","","Alta","dBA","47","49","49"]
["","","","Bassa","dBA","","","45"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32"]
["","Carica","","","kg","0.76","0.76","1.4"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","0.5","0.5","0.9"]
["","GWP","","","","675","675","675"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","15","15","30"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 10m)","0,02 (per lunghezza delle tubazioni superiore ai 10m)","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["","Dislivello","int. - est.","Max.","m","12","12","20"]
["Accessori standard","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1"]
["Alimentazione","Fase","","","","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240"]