{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS25L2V1B","ARXS35L2V1B","ARXS50L2V1B","ARXS60L2V1B","ARXS71L2V1B"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","47","48"]
["","","","Nom.","dBA","","","","49","52"]
["","Raffrescamento","","Alta","dBA","46","48"]
["","","","Nom.","dBA","","","","49","52"]
["Accessori standard","Tappo di scarico","","","","1","1","","1","1"]
["","Manuale di installazione","","","","1","1","","1","1"]
["","Etichetta relativa alla carica di refrigerante","","","","1","","","1","1"]
["","Etichette multilingue sui gas serra fluorurati","","","","1","","","1","1"]
["Refrigerante","Charge","","","TCO2Eq","2.1","2.5"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Carica","","","kg","1.0","1.2","","1.50","1.70"]
["","Tipo","","","","R-410A","R-410A","","R-410A","R-410A"]
["Motore ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","780","780"]
["","","Riscaldamento","Bassissimo","giri/min","740","740"]
["Campo di funzionamento","Raffrescamento","T. esterna","Max.","°CBS","46","46","","46","46"]
["","","","Min.","°CBS","10","10","","-10","-10"]
["","Riscaldamento","T. esterna","Max.","°CBU","18","18","","18","18"]
["","","","Min.","°CBU","-15","-15","","-15","-15"]
["Collegamenti tubazioni","Dislivello","int. - est.","Max.","m","15","15","","20.0","20.0"]
["","Carica di refrigerante aggiuntivo","","","kg/m","0,02 (per lunghezza delle tubazioni superiore ai 10m)","0,02 (per lunghezza delle tubazioni superiore ai 10m)","","0,02 (per lunghezza delle tubazioni superiore ai 10m)","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["Livello potenza sonora","Raffrescamento","","","dBA","","","","62","65"]
["","Riscaldamento","","","dBA","","","","62","65"]
["Compressore","Tipo","","","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing","","Compressore ermetico tipo Swing","Compressore ermetico tipo Swing"]
["Dimensioni","Unità","","Larghezza","mm","765","765","","825","825"]
["","","","Profondità","mm","285","285","","300","300"]
["","","","Altezza","mm","550","550","","735","735"]
["Peso","Unità","","","kg","34","34","","47","47"]
["Ventola","Portata d'aria","Riscaldamento","Bassissimo","cfm","904","904"]
["","","","Bassissimo","m³/min","25.6","25.6"]
["","","Raffrescamento","Bassissimo","m³/min","30.1","30.1"]
["","","","Bassissimo","cfm","1,063","1,063"]
["Power supply","Fase","","","","1~","1~","","1~","1~"]
["","Frequenza","","","Hz","50","50","","50","50"]
["","Tensione","","","V","220-240","220-240","","220-230-240","220-230-240"]
["Note","","","","","(1) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare.","(1) - Se collegato a un’unità esterna multi, consultare le specifiche dell’unità esterna multi da collegare.","(1) - 220V"]
["","","","","","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 230V","(3) - 230V","(3) - 240V"]
["","","","","","(4) - 240V","(4) - 240V"]
["","","","","","(5) - Contiene gas fluorurati a effetto serra","(5) - Contiene gas fluorurati a effetto serra"]
["Ventilatore","Portata d'aria","Raffrescamento","Bassissimo","m³/min","","","48.9"]
["","","Riscaldamento","Bassissimo","m³/min","","","43.1"]
["","","","Bassissimo","cfm","","","1727"]
["","","Riscaldamento","Bassissimo","cfm","","","1522"]
["Dimensioni","Unità","","Altezza","mm","","","735"]
["","","","Larghezza","mm","","","825"]
["","","","Profondità","mm","","","300"]
["Peso","Unità","","","kg","","","47"]
["Motore del ventilatore","Velocità","Raffrescamento","Bassissimo","giri/min","","","670"]
["","","Riscaldamento","Bassissimo","giri/min","","","670"]
["Compressore","Tipo","","","","","","Compressore ermetico tipo Swing"]
["Campo di funzionamento","Raffrescamento","T. esterna","Min.","°CBS","","","10"]
["","","","Max.","°CBS","","","46"]
["","Riscaldamento","T. esterna","Min.","°CBU","","","-15"]
["","","","Max.","°CBU","","","18"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","","","48"]
["","Riscaldamento","","Alta","dBA","","","48"]
["Refrigerante","Tipo","","","","","","R-410A"]
["","Carica","","","kg","","","1.7"]
["","Refrigerante-=-Carica-=-TCO2Eq","","","tCO2Eq","","","3.5"]
["","GWP","","","","","","2087.5"]
["Collegamenti tubazioni","Lunghezza tubazioni","Max.","est. - int.","m","","","30"]
["","Carica di refrigerante aggiuntivo","","","kg/m","","","0,02 (per lunghezza delle tubazioni superiore ai 10m)"]
["","Dislivello","int. - est.","Max.","m","","","20"]
["Accessori standard","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["Alimentazione","Fase","","","","","","1~"]
["","Frequenza","","","Hz","","","50"]
["","Tensione","","","V","","","220-240"]
["Note","","","","","","","","(1) - Contiene gas fluorurati a effetto serra","(1) - Contiene gas fluorurati a effetto serra"]