{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Livello pressione sonora","Riscaldamento","","Alta","dBA","","","","","","43"]
["","","","Medio","dBA","","","","","","35"]
["","","","Funzionamento silenzioso","dBA","","","","","","26"]
["","","","Bassa","dBA","","","","","","29"]
["","Raffrescamento","","Medio","dBA","","","","","","34"]
["","","","Funzionamento silenzioso","dBA","","","","","","20"]
["","","","Bassa","dBA","","","","","","27"]
["","","","Alta","dBA","","","","","","43"]
["Accessori standard","Manuale di installazione","","","","","","","","","1"]
["","Manuale d’uso","","","","","","","","","1"]
["","Telecomando a raggi infrarossi","","","","","","","","","1"]
["","Batterie a secco AA","","","","","","","","","2"]
["","Supporto del telecomando","","","","","","","","","1"]
["","Piastra di montaggio","","","","","","","","","1"]
["","Filtro purificatore d'aria a base di apatite e titanio","","","","","","","","","2"]
["","Viti di fissaggio unità interna","","","","","","","","","2"]
["Sistemi di comando","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Collegamenti tubazioni","Liquido","","DE","mm","","","","","","6.35"]
["","Gas","","DE","mm","","","","","","9.50"]
["","Scarico","","","","","","","","","18"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","","","","","","0.024"]
["","Riscaldamento","","Nom.","kW","","","","","","0.029"]
["Sound power level","Raffrescamento","","","dBA","","","","","","58"]
["","Riscaldamento","","","dBA","","","","","","58"]
["Dimensioni","Unità","","Larghezza","mm","","","","","","770"]
["","","","Profondità","mm","","","","","","225"]
["","","","Altezza","mm","","","","","","286"]
["Rivestimento","Colore","","","","","","","","","Bianco"]
["Peso","Unità","","","kg","","","","","","9.0"]
["Power supply","Fase","","","","","","","","","1~"]
["","Frequenza","","","Hz","","","","","","50"]
["","Nome","","","","","","","","","V1"]
["","Tensione","","","V","","","","","","220-240"]
["Note","","","","","","","","","","(1) - SL: Il livello silent del ventilatore nell'impostazione portata aria"]
["Potenza assorbita","Raffrescamento","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Riscaldamento","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Rivestimento","Colore","","","","Bianco","Bianco","Bianco","Bianco","Bianco"]
["Dimensioni","Unità","","Altezza","mm","286","286","286","286","286"]
["","","","Larghezza","mm","770","770","770","770","770"]
["","","","Profondità","mm","225","225","225","225","225"]
["Peso","Unità","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventilatore","Portata d'aria","Raffrescamento","Alta","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","","","Medio","m³/min","7.8","7.8","8","8","8.2"]
["","","","Bassa","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Funzionamento silenzioso","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Riscaldamento","Alta","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","","","Medio","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","","Bassa","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Funzionamento silenzioso","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Potenza sonora","Raffrescamento","","","dBA","55","55","55","55","58"]
["","Riscaldamento","","","dBA","55","55","55","55","58"]
["Livello pressione sonora","Raffrescamento","","Alta","dBA","39","39","40","40","43"]
["Pressione sonora","Raffrescamento","","Medio","dBA","33","33","33","33","34"]
["Livello pressione sonora","Raffrescamento","","Bassa","dBA","25","25","26","26","27"]
["","","","Funzionamento silenzioso","dBA","20","20","20","20","20"]
["","Riscaldamento","","Alta","dBA","39","39","40","40","43"]
["Pressione sonora","Riscaldamento","","Medio","dBA","34","34","34","34","35"]
["Livello pressione sonora","Riscaldamento","","Bassa","dBA","28","28","28","28","29"]
["","","","Funzionamento silenzioso","dBA","23","23","23","23","26"]
["Attacchi tubazioni","Liquido","","DE","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","DE","mm","9.5","9.5","9.5","9.5","9.5"]
["","Scarico","","","","18","18","18","18","18"]
["Sistemi di comando","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Sistemi di controllo","Telecomando con cavo","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Accessori standard","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Alimentazione","Nome","","","","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~"]
["","Frequenza","","","Hz","50","50","50","50","50"]
["","Tensione","","","V","220-240","220-240","220-240","220-240","220-240"]
["Accessori standard","AAA dry-cell batteries","","","","","2","","2","2"]
["Sistemi di controllo","Telecomando infrarossi","","","","","","ARC480A11","ARC480A11"]
["Accessori standard","Titanium apatite photocatalytic air purification filter","","","","","","2"]