{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-A"]
[]
[]
[]
[]
["","","","","ATXC25AV1B","ATXC35AV1B","ATXC50AV1B","ATXC60AV1B"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","","41"]
["","","Medio","dBA","","34"]
["","","Funzionamento silenzioso","dBA","","22"]
["","","Bassa","dBA","","30"]
["Potenza assorbita","Riscaldamento","Nom.","kW","","1,280"]
["Sound power level","Riscaldamento","","dBA","","54"]
["Dimensioni","Unità","Larghezza","mm","","859"]
["","","Profondità","mm","","209"]
["","","Altezza","mm","","288"]
["Rivestimento","Materiale","","","","Polistirene ad alto impatto"]
["","Colore","","","","Bianco"]
["Peso","Unità","","kg","","9.00"]
["Power supply","Fase","","","","1~"]
["","Frequenza","","Hz","","50"]
["","Tensione","","V","","220-240"]
["Note","","","","","(1) - Il livello di potenza sonora è un valore assoluto che indica la potenza generata da una sorgente sonora."]
["Potenza assorbita","Riscaldamento","Nom.","kW","830","","1550","1810"]
["Rivestimento","Colore","","","Bianco","","Bianco","Bianco"]
["","Materiale","","","Polistirene ad alto impatto","","Polistirene ad alto impatto","Polistirene ad alto impatto"]
["Dimensioni","Unità","Altezza","mm","288","","310","310"]
["","","Larghezza","mm","859","","1120","1120"]
["","","Profondità","mm","209","","237","237"]
["Peso","Unità","","kg","9.00","","14.0","14.0"]
["Potenza sonora","Riscaldamento","","dBA","53","","53","61"]
["Livello pressione sonora","Riscaldamento","Alta","dBA","40","","40","43"]
["Pressione sonora","Riscaldamento","Medio","dBA","34","","38","41"]
["Livello pressione sonora","Riscaldamento","Bassa","dBA","29","","35","37"]
["","","Funzionamento silenzioso","dBA","21","","32","33"]
["Alimentazione","Fase","","","1~","","1~","1~"]
["","Frequenza","","Hz","50","","50","50"]
["","Tensione","","V","220-240","","220-240","220-240"]